(module SolderJumper-3_Open (layer F.Cu) (tedit 5F2ECD05)
  (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
  (tags "solder jumper open")
  (attr virtual)
  (fp_text reference JP1 (at 0 -1.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TMS (at 0 2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.77 0.7) (end -0.47 1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.1 1) (end -0.5 1) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.8 0.7) (end -1.1 1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.15 0.5) (end -1.15 -0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.15 0.5) (end -1.15 0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.15 -0.5) (end 1.15 0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.15 -0.5) (end 1.15 -0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.25 -0.6) (end 1.25 -0.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.25 -0.6) (end -1.25 0.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.25 0.6) (end 1.25 -0.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.25 0.6) (end -1.25 0.6) (layer F.CrtYd) (width 0.05))
  (pad 3 smd oval (at 0.7 0) (size 0.5 0.6) (layers F.Cu F.Mask))
  (pad 2 smd roundrect (at 0 0) (size 0.5 0.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -0.7 0) (size 0.5 0.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
)
