# User Direct Video DAC Configuration File
# This file allows users to add their own DAC configurations
# or override settings from dv_dac.txt
#
# Format: mfg_id,hdmi_limited,hdmi_audio_96k,composite_sync,name
# 
# mfg_id: Manufacturer ID from EDID bytes 0x08-0x09 (hex, e.g. 0x48F4)
#         This is the raw 16-bit value from EDID, NOT the decoded 3-letter code
# hdmi_limited: 0=full range RGB (0-255)
#               1=limited range RGB (16-235) 
#               2=limited range RGB (16-255)
# hdmi_audio_96k: 0=48kHz audio, 1=96kHz audio
# composite_sync: 0=disable composite sync, 1=enable composite sync, blank=use MiSTer.ini setting
# name: Description of the DAC (optional, for logging purposes)
#
# The mfg_id comes from EDID bytes:
#   Byte 0x08: High byte of manufacturer ID
#   Byte 0x09: Low byte of manufacturer ID
#   Combined as: (byte_08 << 8) | byte_09
#
# Examples:
# 0x40D8,0,1,,PixelFX Morph (full range, use MiSTer.ini csync setting)
# 0x1234,1,1,1,Custom DAC (limited 16-235, force composite sync on)
# 0x5678,2,0,0,Another DAC (limited 16-255, force composite sync off)
#
# Note: Entries in this file will override any matching mfg_id from dv_dac.txt
#
# Known video upscalers that support direct video
# (remove "# " in front of device if you want to use automatic direct video mode):
# 0x40D8,0,1,1,PixelFX Morph 4K
# 0x4A8B,0,1,1,RetroTink 4K Pro
