(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ESP32" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 43.18 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32" (id 1) (at 0 -41.91 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 6.35 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32_datasheet_en.pdf" (id 3) (at 6.35 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "esp32 soc wifi bluetooth ethernet" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ESP32 is a single 2.4 GHz Wi-Fi-and-Bluetooth combo chip designed with the TSMC ultra-low-power 40 nmtechnology." (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32_0_0"
      (text "ESP32" (at 1.27 0 0)
        (effects (font (size 2.54 2.54)))
      )
    )
    (symbol "ESP32_0_1"
      (rectangle (start -34.29 41.91) (end 35.56 -40.64)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32_1_1"
      (pin power_in line (at -36.83 -33.02 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 30.48 0) (length 2.54)
        (name "VDET_1/GPIO34/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 27.94 0) (length 2.54)
        (name "VDET_2/GPIO35/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 13.97 0) (length 2.54)
        (name "32K_XP/GPIO32/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 11.43 0) (length 2.54)
        (name "32K_XN/GPIO33/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -2.54 180) (length 2.54)
        (name "GPIO25/ADC2_CH8/DAC_1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -5.08 180) (length 2.54)
        (name "GPIO26/ADC2_CH9/DAC_2" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -7.62 180) (length 2.54)
        (name "GPIO27/ADC2_CH7" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 -8.89 0) (length 2.54)
        (name "MTMS/GPIO14/ADC2_CH6" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 -11.43 0) (length 2.54)
        (name "MTDI/GPIO12/ADC2_CH5" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -27.94 0) (length 2.54)
        (name "VDD3P3_RTC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 39.37 0) (length 2.54)
        (name "LNA_IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 -13.97 0) (length 2.54)
        (name "MTCK/GPIO13/ADC2_CH4" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 -16.51 0) (length 2.54)
        (name "MTDO/GPIO15/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 22.86 180) (length 2.54)
        (name "GPIO2/ADC2_CH2" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 25.4 180) (length 2.54)
        (name "GPIO0/BOOT/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 20.32 180) (length 2.54)
        (name "GPIO4/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -31.75 180) (length 2.54)
        (name "GPIO16" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 38.1 -13.97 180) (length 2.54)
        (name "VDD_SDIO" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -34.29 180) (length 2.54)
        (name "GPIO17" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -24.13 180) (length 2.54)
        (name "SD_DATA_2/GPIO9" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -26.67 180) (length 2.54)
        (name "SD_DATA_3/GPIO10" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -20.32 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -29.21 180) (length 2.54)
        (name "SD_CMD/GPIO11" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -16.51 180) (length 2.54)
        (name "SD_CLK/GPIO6" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -19.05 180) (length 2.54)
        (name "SD_DATA_0/GPIO7" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -21.59 180) (length 2.54)
        (name "SD_DATA_1/GPIO8" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 17.78 180) (length 2.54)
        (name "GPIO5" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 10.16 180) (length 2.54)
        (name "GPIO18" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 0 180) (length 2.54)
        (name "GPIO23" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -25.4 0) (length 2.54)
        (name "VDD3P3_CPU" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 7.62 180) (length 2.54)
        (name "GPIO19" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 2.54 180) (length 2.54)
        (name "GPIO22" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -22.86 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 30.48 180) (length 2.54)
        (name "U0RXD/GPIO3" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 33.02 180) (length 2.54)
        (name "U0TXD/GPIO1" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 5.08 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -35.56 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -36.83 6.35 0) (length 2.54)
        (name "XTAL_N" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 3.81 0) (length 2.54)
        (name "XTAL_P" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -38.1 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 -3.81 0) (length 2.54)
        (name "CAP2" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 -1.27 0) (length 2.54)
        (name "CAP1" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 38.1 -38.1 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 25.4 0) (length 2.54)
        (name "SENSOR_VP/GPIO36/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 22.86 0) (length 2.54)
        (name "SENSOR_CAPP/GPIO37/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 20.32 0) (length 2.54)
        (name "SENSOR_CAPN/GPIO38/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 17.78 0) (length 2.54)
        (name "SENSOR_VN/GPIO39/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 34.29 0) (length 2.54)
        (name "CHIP_PU" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-C3" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-C3" (id 1) (at 0 -27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm" (id 2) (at 36.83 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c3_datasheet_en.pdf" (id 3) (at 36.83 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ESP32-C3 family is an ultra-low-power MCU-based SoC solution that supports 2.4 GHz Wi-Fi and Bluetooth®Low Energy (Bluetooth LE)." (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-C3_0_0"
      (text "ESP32-C3" (at 1.27 -24.13 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin bidirectional line (at -27.94 27.94 0) (length 2.54)
        (name "LNA_IN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 2.54 0) (length 2.54)
        (name "MTDI/GPIO5/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -21.59 0) (length 2.54)
        (name "VDD3P3_RTC" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 0 0) (length 2.54)
        (name "MTCK/GPIO6" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 -2.54 0) (length 2.54)
        (name "MTDO/GPIO7" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -12.7 180) (length 2.54)
        (name "GPIO8" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -10.16 180) (length 2.54)
        (name "GPIO9/BOOT" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -7.62 180) (length 2.54)
        (name "GPIO10" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -24.13 0) (length 2.54)
        (name "VDD3P3_CPU" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -5.08 180) (length 2.54)
        (name "VDD_SPI/GPIO11" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -2.54 180) (length 2.54)
        (name "SPIHD/GPIO12" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -16.51 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 0 180) (length 2.54)
        (name "SPIWP/GPIO13" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 2.54 180) (length 2.54)
        (name "SPICS0/GPIO14" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 5.08 180) (length 2.54)
        (name "SPICLK/GPIO15" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 7.62 180) (length 2.54)
        (name "SPID/GPIO16" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 10.16 180) (length 2.54)
        (name "SPIQ/GPIO17" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 16.51 180) (length 2.54)
        (name "GPIO18/USB_D-" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 19.05 180) (length 2.54)
        (name "GPIO19/USB_D+" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 25.4 180) (length 2.54)
        (name "U0RXD/GPIO20" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 27.94 180) (length 2.54)
        (name "U0TXD/GPIO21" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -27.94 12.7 0) (length 2.54)
        (name "XTAL_N" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -19.05 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -27.94 10.16 0) (length 2.54)
        (name "XTAL_P" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -11.43 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -8.89 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 -24.13 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -27.94 20.32 0) (length 2.54)
        (name "XTAL_32K_P/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -27.94 17.78 0) (length 2.54)
        (name "XTAL_32K_N/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -17.78 180) (length 2.54)
        (name "GPIO2/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -27.94 24.13 0) (length 2.54)
        (name "CHIP_EN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -15.24 180) (length 2.54)
        (name "GPIO3/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 5.08 0) (length 2.54)
        (name "MTMS/GPIO4/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ESP32-C3_0_1"
      (rectangle (start -25.4 30.48) (end 25.4 -26.67)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
  )
  (symbol "ESP32-C3-MINI-1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 33.02 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-C3-MINI-1" (id 1) (at 0 -30.48 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-C3-MINI-1" (id 2) (at 0 -33.02 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c3-mini-1_datasheet_en.pdf" (id 3) (at -62.23 -33.02 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "esp32-c3" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ESP32-C3-MINI-1 is a general-purpose Wi-Fi and Bluetooth LE module. This module features a rich set of peripherals and a small size, which makes it an ideal choice for smart home, industrial automation, health care, consumer electronics, etc" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-C3-MINI-1_0_0"
      (text "ESP32-C3-MINI-1" (at 1.27 27.94 0)
        (effects (font (size 2.54 2.54)))
      )
    )
    (symbol "ESP32-C3-MINI-1_0_1"
      (rectangle (start -24.13 31.75) (end 25.4 -29.21)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32-C3-MINI-1_1_1"
      (pin power_in line (at 27.94 -16.51 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 13.97 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 -21.59 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 11.43 0) (length 2.54)
        (name "GPIO0/ADC1_CH0/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 8.89 0) (length 2.54)
        (name "GPIO1/ADC1_CH1/XTAL_32K_N" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 -24.13 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 11.43 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 6.35 0) (length 2.54)
        (name "GPIO10" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 8.89 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 3.81 0) (length 2.54)
        (name "GPIO4/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 1.27 0) (length 2.54)
        (name "GPIO5/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 -19.05 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -1.27 0) (length 2.54)
        (name "GPIO6" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -3.81 0) (length 2.54)
        (name "GPIO7" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -6.35 0) (length 2.54)
        (name "GPIO8" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -8.89 0) (length 2.54)
        (name "GPIO9" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 6.35 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 3.81 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -11.43 0) (length 2.54)
        (name "GPIO18/USB_D-" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -13.97 0) (length 2.54)
        (name "GPIO19/USB_D+" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 1.27 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 -1.27 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -26.67 -26.67 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -19.05 0) (length 2.54)
        (name "GPIO20/U0RXD" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -21.59 0) (length 2.54)
        (name "GPIO21/U0TXD" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 -3.81 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 -6.35 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 -8.89 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 -11.43 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 -26.67 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 21.59 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 16.51 0) (length 2.54)
        (name "GPIO2/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 13.97 0) (length 2.54)
        (name "GPIO3/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 19.05 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -26.67 21.59 0) (length 2.54)
        (name "EN/CHIP_PU" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 27.94 16.51 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-C3-WROOM-02" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 33.02 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-C3-WROOM-02" (id 1) (at 0 -30.48 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-C3-WROOM-02" (id 2) (at 0 -33.02 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c3-wroom-02_datasheet_en.pdf" (id 3) (at -62.23 -33.02 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "esp32-c3 module" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ESP32-C3-WROOM-02 is a general-purpose Wi-Fi and Bluetooth LE module. This module features a rich set of peripherals and high performance, which makes it an ideal choice for smart home, industrial automation, health care, consumer electronics, etc." (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-C3-WROOM-02_0_0"
      (text "ESP32-C3-WROOM-02" (at 1.27 27.94 0)
        (effects (font (size 2.54 2.54)))
      )
    )
    (symbol "ESP32-C3-WROOM-02_0_1"
      (rectangle (start -24.13 31.75) (end 25.4 -29.21)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32-C3-WROOM-02_1_1"
      (pin power_in line (at -26.67 -26.67 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -13.97 0) (length 2.54)
        (name "GPIO10" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 16.51 180) (length 2.54)
        (name "GPIO20/U0RXD" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 13.97 180) (length 2.54)
        (name "GPIO21/U0TXD" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 8.89 180) (length 2.54)
        (name "GPIO18/USB_D-" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 6.35 180) (length 2.54)
        (name "GPIO19/USB_D+" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 8.89 0) (length 2.54)
        (name "GPIO3/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 11.43 0) (length 2.54)
        (name "GPIO2/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 13.97 0) (length 2.54)
        (name "GPIO1/ADC1_CH1/XTAL_32K_N" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 16.51 0) (length 2.54)
        (name "GPIO0/ADC1_CH0/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 -26.67 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -26.67 21.59 0) (length 2.54)
        (name "EN/CHIP_PU" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 6.35 0) (length 2.54)
        (name "GPIO4/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 3.81 0) (length 2.54)
        (name "GPIO5/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -3.81 0) (length 2.54)
        (name "GPIO6" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -6.35 0) (length 2.54)
        (name "GPIO7" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -8.89 0) (length 2.54)
        (name "GPIO8" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -26.67 -11.43 0) (length 2.54)
        (name "GPIO9" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 -24.13 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-DevKitC" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -8.89 26.67 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-DevKitC" (id 1) (at 0 -29.21 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-DevKitC" (id 2) (at 0 -31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://docs.espressif.com/projects/esp-idf/zh_CN/latest/esp32/hw-reference/esp32/get-started-devkitc.html" (id 3) (at 3.81 -31.75 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "ESP32" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Development Kit" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-DevKitC_0_0"
      (pin power_in line (at -33.02 -11.43 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -33.02 -24.13 0) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ESP32-DevKitC_0_1"
      (rectangle (start -30.48 25.4) (end 34.29 -27.94)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32-DevKitC_1_1"
      (pin power_in line (at -33.02 21.59 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 -1.27 0) (length 2.54)
        (name "DAC_2/ADC2_CH9/GPIO26" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 -3.81 0) (length 2.54)
        (name "ADC2_CH7/GPIO27" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 -6.35 0) (length 2.54)
        (name "MTMS/GPIO14/ADC2_CH6" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 -8.89 0) (length 2.54)
        (name "*MTDI/GPIO12/ADC2_CH5" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 -13.97 0) (length 2.54)
        (name "MTCK/GPIO13/ADC2_CH4" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 -16.51 0) (length 2.54)
        (name "SD_DATA2/GPIO9" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 -19.05 0) (length 2.54)
        (name "SD_DATA3/GPIO10" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 -21.59 0) (length 2.54)
        (name "CMD" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -33.02 19.05 0) (length 2.54)
        (name "CHIP_PU" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -24.13 180) (length 2.54)
        (name "SD_CLK/GPIO6" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -21.59 180) (length 2.54)
        (name "SD_DATA0/GPIO7" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -19.05 180) (length 2.54)
        (name "SD_DATA1/GPIO8" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -16.51 180) (length 2.54)
        (name "*MTDO/GPIO15/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -13.97 180) (length 2.54)
        (name "ADC2_CH2/*GPIO2" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -11.43 180) (length 2.54)
        (name "*GPIO0/BOOT/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -8.89 180) (length 2.54)
        (name "ADC2_CH0/GPIO4" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -6.35 180) (length 2.54)
        (name "GPIO16" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -3.81 180) (length 2.54)
        (name "GPIO17" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -1.27 180) (length 2.54)
        (name "*GPIO5" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -33.02 16.51 0) (length 2.54)
        (name "SENSOR_VP/GPIO36/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 1.27 180) (length 2.54)
        (name "GPIO18" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 3.81 180) (length 2.54)
        (name "GPIO19" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 36.83 6.35 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 8.89 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 11.43 180) (length 2.54)
        (name "U0RXD/GPIO3" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 13.97 180) (length 2.54)
        (name "U0TXD/GPIO1" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 16.51 180) (length 2.54)
        (name "GPIO22" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 19.05 180) (length 2.54)
        (name "GPIO23" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 36.83 21.59 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -33.02 13.97 0) (length 2.54)
        (name "SENSOR_VN/GPIO39/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -33.02 11.43 0) (length 2.54)
        (name "VDET_1/GPIO34/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -33.02 8.89 0) (length 2.54)
        (name "VDET_2/GPIO35/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 6.35 0) (length 2.54)
        (name "32K_XP/GPIO32/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 3.81 0) (length 2.54)
        (name "32K_XN/GPIO33/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -33.02 1.27 0) (length 2.54)
        (name "DAC_1/ADC2_CH8/GPIO25" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-PICO-V3" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 43.18 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-PICO-V3" (id 1) (at 0 -41.91 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm" (id 2) (at 0 -44.45 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32_datasheet_en.pdf" (id 3) (at 6.35 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "The ESP32-PICO-V3 is a System-in-Package (SiP) device that is based on ESP32 with ECO V3 wafer, providingcomplete Wi-Fi and Bluetooth®functionalities. It integrates a 4 MB SPI flash." (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-PICO-V3_0_0"
      (text "ESP32-PICO-V3" (at 0 3.81 0)
        (effects (font (size 2.54 2.54)))
      )
    )
    (symbol "ESP32-PICO-V3_0_1"
      (rectangle (start -34.29 41.91) (end 35.56 -40.64)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32-PICO-V3_1_1"
      (pin power_in line (at -36.83 -33.02 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 30.48 0) (length 2.54)
        (name "VDET_1/GPIO34/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 27.94 0) (length 2.54)
        (name "VDET_2/GPIO35/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 13.97 0) (length 2.54)
        (name "32K_XP/GPIO32/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 11.43 0) (length 2.54)
        (name "32K_XN/GPIO33/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -2.54 180) (length 2.54)
        (name "GPIO25/ADC2_CH8/DAC_1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -5.08 180) (length 2.54)
        (name "GPIO26/ADC2_CH9/DAC_2" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -7.62 180) (length 2.54)
        (name "GPIO27/ADC2_CH7" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 -8.89 0) (length 2.54)
        (name "MTMS/GPIO14/ADC2_CH6" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 -11.43 0) (length 2.54)
        (name "*MTDI/GPIO12/ADC2_CH5" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -30.48 0) (length 2.54)
        (name "VDD3P3_RTC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 39.37 0) (length 2.54)
        (name "LNA_IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 -13.97 0) (length 2.54)
        (name "MTCK/GPIO13/ADC2_CH4" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -36.83 -16.51 0) (length 2.54)
        (name "*MTDO/GPIO15/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 22.86 180) (length 2.54)
        (name "*GPIO2/ADC2_CH2" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 25.4 180) (length 2.54)
        (name "*GPIO0/BOOT/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 20.32 180) (length 2.54)
        (name "GPIO4/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 38.1 -31.75 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 38.1 -13.97 180) (length 2.54)
        (name "VDD_SDIO" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -34.29 180) (length 2.54)
        (name "GPIO20" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -24.13 180) (length 2.54)
        (name "SD_DATA_2/GPIO9" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -26.67 180) (length 2.54)
        (name "SD_DATA_3/GPIO10" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -22.86 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -29.21 180) (length 2.54)
        (name "SD_CMD/GPIO11" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -16.51 180) (length 2.54)
        (name "SD_CLK/GPIO6" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -19.05 180) (length 2.54)
        (name "SD_DATA_0/GPIO7" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 -21.59 180) (length 2.54)
        (name "SD_DATA_1/GPIO8" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 17.78 180) (length 2.54)
        (name "*GPIO5" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 38.1 10.16 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 38.1 0 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -27.94 0) (length 2.54)
        (name "VDD3P3_CPU" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 7.62 180) (length 2.54)
        (name "GPIO19" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 2.54 180) (length 2.54)
        (name "GPIO22" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -25.4 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 30.48 180) (length 2.54)
        (name "U0RXD/GPIO3" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 33.02 180) (length 2.54)
        (name "U0TXD/GPIO1" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 38.1 5.08 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -35.56 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -36.83 6.35 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -36.83 3.81 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -36.83 -38.1 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -36.83 -3.81 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -36.83 -1.27 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 38.1 -38.1 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 25.4 0) (length 2.54)
        (name "SENSOR_VP/GPIO36/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 22.86 0) (length 2.54)
        (name "SENSOR_CAPP/GPIO37/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 20.32 0) (length 2.54)
        (name "SENSOR_CAPN/GPIO38/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 17.78 0) (length 2.54)
        (name "SENSOR_VN/GPIO39/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -36.83 34.29 0) (length 2.54)
        (name "CHIP_PU" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-S2" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 44.45 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-S2" (id 1) (at 0 -45.72 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm" (id 2) (at 0 -48.26 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s2_datasheet_en.pdf" (id 3) (at -2.54 8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ESP32-S2 family is a highly-integrated, low-power, 2.4GHz Wi-Fi System-on-Chip (SoC) solution." (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S2_0_0"
      (text "ESP32-S2" (at 0 0 0)
        (effects (font (size 2.54 2.54)))
      )
    )
    (symbol "ESP32-S2_0_1"
      (rectangle (start -33.02 43.18) (end 34.29 -44.45)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32-S2_1_1"
      (pin power_in line (at -35.56 -41.91 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 22.86 0) (length 2.54)
        (name "GPIO5/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 20.32 0) (length 2.54)
        (name "GPIO6/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 17.78 0) (length 2.54)
        (name "GPIO7/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 15.24 0) (length 2.54)
        (name "GPIO8/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 12.7 0) (length 2.54)
        (name "GPIO9/ADC1_CH8" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 10.16 0) (length 2.54)
        (name "GPIO10/ADC1_CH9" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 7.62 0) (length 2.54)
        (name "GPIO11/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 5.08 0) (length 2.54)
        (name "GPIO12/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 2.54 0) (length 2.54)
        (name "GPIO13/ADC2_CH2" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 0 0) (length 2.54)
        (name "GPIO14/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 40.64 0) (length 2.54)
        (name "LNA_IN/RF" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -29.21 0) (length 2.54)
        (name "VDD3P3_RTC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional clock (at -35.56 -5.08 0) (length 2.54)
        (name "GPIO15/ADC2_CH4/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional clock (at -35.56 -7.62 0) (length 2.54)
        (name "GPIO16/ADC2_CH5/XTAL_32K_N" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -33.02 180) (length 2.54)
        (name "GPIO17/ADC2_CH6/DAC_1" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -35.56 180) (length 2.54)
        (name "GPIO18/ADC2_CH7/DAC_2" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -6.35 180) (length 2.54)
        (name "GPIO19/ADC2_CH8/USB_D-" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -3.81 180) (length 2.54)
        (name "GPIO20/ADC2_CH9/USB_D+" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -26.67 0) (length 2.54)
        (name "VDD3P3_RTC_IO" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 1.27 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 3.81 180) (length 2.54)
        (name "SPI_CS1/GPIO26" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -34.29 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -24.13 0) (length 2.54)
        (name "VDD_SPI" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 6.35 180) (length 2.54)
        (name "SPIHD/GPIO27" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 8.89 180) (length 2.54)
        (name "SPIWP/GPIO28" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 11.43 180) (length 2.54)
        (name "SPICS0/GPIO29" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 13.97 180) (length 2.54)
        (name "SPICLK/GPIO30" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 16.51 180) (length 2.54)
        (name "SPIQ/GPIO31" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 19.05 180) (length 2.54)
        (name "SPID/GPIO32" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 21.59 180) (length 2.54)
        (name "GPIO33" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 24.13 180) (length 2.54)
        (name "GPIO34" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 26.67 180) (length 2.54)
        (name "GPIO35" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -31.75 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 29.21 180) (length 2.54)
        (name "GPIO36" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 31.75 180) (length 2.54)
        (name "GPIO37" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 34.29 180) (length 2.54)
        (name "GPIO38" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 36.83 -19.05 180) (length 2.54)
        (name "MTCK/JTAG/GPIO39" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 36.83 -16.51 180) (length 2.54)
        (name "MTDO/JTAG/GPIO40" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -21.59 0) (length 2.54)
        (name "VDD3P3_CPU" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 36.83 -13.97 180) (length 2.54)
        (name "MTDI/JTAG/GPIO41" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 36.83 -11.43 180) (length 2.54)
        (name "MTMS/JTAG/GPIO42" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 38.1 180) (length 2.54)
        (name "U0TXD/GPIO43" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 40.64 180) (length 2.54)
        (name "U0RXD/GPIO44" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -27.94 180) (length 2.54)
        (name "GPIO0/BOOT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -25.4 180) (length 2.54)
        (name "GPIO45" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -39.37 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional clock (at -35.56 -12.7 0) (length 2.54)
        (name "XTAL_N" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional clock (at -35.56 -15.24 0) (length 2.54)
        (name "XTAL_P" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -36.83 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 36.83 -22.86 180) (length 2.54)
        (name "GPIO46" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 36.83 0) (length 2.54)
        (name "CHIP_PU/RESET" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 36.83 -41.91 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 33.02 0) (length 2.54)
        (name "GPIO1/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 30.48 0) (length 2.54)
        (name "GPIO2/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 27.94 0) (length 2.54)
        (name "GPIO3/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 25.4 0) (length 2.54)
        (name "GPIO4/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-S2-MINI-1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 46.99 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-S2-MINI-1" (id 1) (at 0 -43.18 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-S2-MINI-1" (id 2) (at 0 -45.72 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s2-mini-1_esp32-s2-mini-1u_datasheet_en.pdf" (id 3) (at -1.27 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "ESP32-S2" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ESP32-S2-MINI-1 and ESP32-S2-MINI-1U are two powerful, generic Wi-Fi MCU modules that have a rich set of peripherals. They are an ideal choice for a wide variety of application scenarios relating to Internet of Things (IoT), wearable electronics and smart home." (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S2-MINI-1_0_0"
      (pin power_in line (at -35.56 -36.83 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 36.83 17.78 180) (length 2.54)
        (name "GPIO46" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 43.18 0) (length 2.54)
        (name "CHIP/PU/RESET" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -39.37 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ESP32-S2-MINI-1_1_1"
      (rectangle (start -33.02 -41.91) (end 34.29 45.72)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "ESP32-S2-MINI-1" (at -1.27 -35.56 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin power_in line (at -35.56 -26.67 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 22.86 0) (length 2.54)
        (name "GPIO6/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 20.32 0) (length 2.54)
        (name "GPIO7/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 17.78 0) (length 2.54)
        (name "GPIO8/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 15.24 0) (length 2.54)
        (name "GPIO9/ADC1_CH8" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 12.7 0) (length 2.54)
        (name "GPIO10/ADC1_CH9" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 10.16 0) (length 2.54)
        (name "GPIO11/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 7.62 0) (length 2.54)
        (name "GPIO12/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 5.08 0) (length 2.54)
        (name "GPIO13/ADC2_CH2" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 2.54 0) (length 2.54)
        (name "GPIO14/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 -7.62 0) (length 2.54)
        (name "GPIO15/ADC2_CH4/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -29.21 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 -13.97 0) (length 2.54)
        (name "GPIO16/ADC2_CH5/XTAL_32K_N" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -29.21 180) (length 2.54)
        (name "ADC2_CH7/DAC_2/GPIO17" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -26.67 180) (length 2.54)
        (name "ADC2_CH6/DAC_1/GPIO18" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 0 180) (length 2.54)
        (name "USB_D-/ADC2_CH8/GPIO19" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 2.54 180) (length 2.54)
        (name "USB_D+/ADC2_CH9/GPIO20" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 7.62 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 10.16 180) (length 2.54)
        (name "SPI_CS1/GPIO26" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 36.83 -36.83 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 22.86 180) (length 2.54)
        (name "GPIO33" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 25.4 180) (length 2.54)
        (name "GPIO34" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -20.32 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -31.75 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 27.94 180) (length 2.54)
        (name "GPIO35" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 30.48 180) (length 2.54)
        (name "GPIO36" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 33.02 180) (length 2.54)
        (name "GPIO37" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 35.56 180) (length 2.54)
        (name "GPIO38" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -12.7 180) (length 2.54)
        (name "MTCK/JTAG/GPIO39" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -10.16 180) (length 2.54)
        (name "MTDO/JTAG/GPIO40" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -7.62 180) (length 2.54)
        (name "MTDI/JTAG/GPIO41" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -5.08 180) (length 2.54)
        (name "MTMS/JTAG/GPIO42" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 40.64 180) (length 2.54)
        (name "GPIO43/U0TXD/PROG" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -21.59 180) (length 2.54)
        (name "GPIO0/BOOT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 43.18 180) (length 2.54)
        (name "GPIO44/U0RXD/PROG" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -19.05 180) (length 2.54)
        (name "GPIO45" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -34.29 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 35.56 0) (length 2.54)
        (name "GPIO1/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 33.02 0) (length 2.54)
        (name "GPIO2/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 30.48 0) (length 2.54)
        (name "GPIO3/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 27.94 0) (length 2.54)
        (name "GPIO4/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 25.4 0) (length 2.54)
        (name "GPIO5/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-S2-SOLO" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 43.18 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-S2-SOLO" (id 1) (at 0 -46.99 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-S2-SOLO" (id 2) (at 0 -49.53 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s2-solo_esp32-s2-solo-u_datasheet_en.pdf" (id 3) (at 6.35 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "esp32-s2 solo" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ESP32-S2-SOLO and ESP32-S2-SOLO-U are two powerful, generic Wi-Fi MCU modules that have a rich set of peripherals." (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S2-SOLO_0_1"
      (rectangle (start -40.64 41.91) (end 40.64 -45.72)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32-S2-SOLO_1_1"
      (text "ESP32-S2-SOLO" (at 0 -36.83 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin power_in line (at 43.18 -38.1 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -19.05 0) (length 2.54)
        (name "GPIO17/U1TXD/ADC2_CH6/DAC_1" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -21.59 0) (length 2.54)
        (name "GPIO18/U1RXD/ADC2_CH7/DAC_2/CLK_OUT3" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 3.81 0) (length 2.54)
        (name "GPIO8/TOUCH8/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -24.13 0) (length 2.54)
        (name "GPIO19/U1RTS/ADC2_CH8/CLK_OUT2/USB_D-" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -26.67 0) (length 2.54)
        (name "GPIO20/U1CTS/ADC2_CH9/CLK_OUT1/USB_D+" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 16.51 0) (length 2.54)
        (name "GPIO3/TOUCH3/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 43.18 -6.35 180) (length 2.54)
        (name "GPIO46" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 1.27 0) (length 2.54)
        (name "GPIO9/TOUCH9/ADC1_CH8/FSPIHD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -1.27 0) (length 2.54)
        (name "GPIO10/TOUCH10/ADC1_CH9/FSPICS0/FSPIIO4" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -3.81 0) (length 2.54)
        (name "GPIO11/TOUCH11/ADC2_CH0/FSPID/FSPIIO5" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -43.18 -40.64 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -6.35 0) (length 2.54)
        (name "GPIO12/TOUCH12/ADC2_CH1/FSPICLK/FSPIIO6" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -8.89 0) (length 2.54)
        (name "GPIO13/TOUCH13/ADC2_CH2/FSPIQ/FSPIIO7" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -11.43 0) (length 2.54)
        (name "GPIO14/TOUCH14/ADC2_CH3/FSPIWP/FSPIDQS" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -29.21 0) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 27.94 180) (length 2.54)
        (name "SPIIO4/GPIO33/FSPIHD" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 25.4 180) (length 2.54)
        (name "SPIIO5/GPIO34/FSPICS0" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 -3.81 180) (length 2.54)
        (name "GPIO45" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 24.13 0) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 22.86 180) (length 2.54)
        (name "SPIIO6/GPIO35/FSPID" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 20.32 180) (length 2.54)
        (name "SPIIO7/GPIO36/FSPICLK" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 38.1 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 17.78 180) (length 2.54)
        (name "SPIDQS/GPIO37/FSPIQ" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 15.24 180) (length 2.54)
        (name "GPIO38/FSPIWP" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 7.62 180) (length 2.54)
        (name "MTCK/GPIO39/CLK_OUT3" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 5.08 180) (length 2.54)
        (name "MTDO/GPIO40/CLK_OUT2" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 2.54 180) (length 2.54)
        (name "MTDI/GPIO41/CLK_OUT1" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 0 180) (length 2.54)
        (name "MTMS/GPIO42" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 38.1 180) (length 2.54)
        (name "U0RXD/GPIO44/CLK_OUT2" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.18 35.56 180) (length 2.54)
        (name "U0TXD/GPIO43/CLK_OUT1" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 19.05 0) (length 2.54)
        (name "GPIO2/TOUCH2/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 21.59 0) (length 2.54)
        (name "GPIO1/TOUCH1/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 13.97 0) (length 2.54)
        (name "GPIO4/TOUCH4/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 43.18 -40.64 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 43.18 -43.18 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 11.43 0) (length 2.54)
        (name "GPIO5/TOUCH5/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 8.89 0) (length 2.54)
        (name "GPIO6/TOUCH6/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 6.35 0) (length 2.54)
        (name "GPIO7/TOUCH7/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -13.97 0) (length 2.54)
        (name "GPIO15/U0RTS/ADC2_CH4/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -43.18 -16.51 0) (length 2.54)
        (name "GPIO16/U0CTS/ADC2_CH5/XTAL_32K_N" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-S2-Saola-1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-S2-Saola-1" (id 1) (at 0 -31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-S2-Saola-1" (id 2) (at 0 -34.29 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 24.13 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "ESP32-S2" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Development Kit" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S2-Saola-1_0_0"
      (text "ESP32-S2-Saola-1" (at 0 24.13 0)
        (effects (font (size 2.0066 2.0066)))
      )
      (pin power_in line (at -34.29 24.13 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 1.27 0) (length 2.54)
        (name "GPIO8/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -1.27 0) (length 2.54)
        (name "GPIO9/ADC1_CH8" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -3.81 0) (length 2.54)
        (name "GPIO10/ADC1_CH9" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -6.35 0) (length 2.54)
        (name "GPIO11/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -8.89 0) (length 2.54)
        (name "GPIO12/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -11.43 0) (length 2.54)
        (name "GPIO13/ADC2_CH2" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -13.97 0) (length 2.54)
        (name "GPIO14/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -16.51 0) (length 2.54)
        (name "GPIO15/ADC2_CH4/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -19.05 0) (length 2.54)
        (name "GPIO16/ADC2_CH5/XTAL_32K_N" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -21.59 0) (length 2.54)
        (name "ADC2_CH7/DAC_2/GPIO17" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 21.59 0) (length 2.54)
        (name "GPIO0/BOOT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -34.29 -24.13 0) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -34.29 -26.67 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -26.67 180) (length 2.54)
        (name "ADC2_CH6/DAC_1/GPIO18" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -24.13 180) (length 2.54)
        (name "USB_D-/ADC2_CH8/GPIO19" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -21.59 180) (length 2.54)
        (name "USB_D+/ADC2_CH9/GPIO20" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -19.05 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -16.51 180) (length 2.54)
        (name "SPI_CS1/GPIO26" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -13.97 180) (length 2.54)
        (name "GPIO33" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -11.43 180) (length 2.54)
        (name "GPIO34" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -8.89 180) (length 2.54)
        (name "GPIO35" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 19.05 0) (length 2.54)
        (name "GPIO1/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -6.35 180) (length 2.54)
        (name "GPIO36" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -3.81 180) (length 2.54)
        (name "GPIO37" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -1.27 180) (length 2.54)
        (name "GPIO38" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 1.27 180) (length 2.54)
        (name "MTCK/JTAG/GPIO39" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 3.81 180) (length 2.54)
        (name "MTDI/JTAG/GPIO41" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 6.35 180) (length 2.54)
        (name "MTDO/JTAG/GPIO40" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 8.89 180) (length 2.54)
        (name "MTMS/JTAG/GPIO42" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 11.43 180) (length 2.54)
        (name "GPIO43/U0TXD/PROG" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 13.97 180) (length 2.54)
        (name "GPIO44/U0RXD/PROG" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 16.51 180) (length 2.54)
        (name "*VDD_SPI/GPIO45" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at -34.29 16.51 0) (length 2.54)
        (name "GPIO2/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 36.83 19.05 180) (length 2.54)
        (name "GPIO46" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 36.83 21.59 180) (length 2.54)
        (name "CHIP/PU/RESET" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 36.83 24.13 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 13.97 0) (length 2.54)
        (name "GPIO3/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 11.43 0) (length 2.54)
        (name "GPIO4/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 8.89 0) (length 2.54)
        (name "GPIO5/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 6.35 0) (length 2.54)
        (name "GPIO6/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 3.81 0) (length 2.54)
        (name "GPIO7/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ESP32-S2-Saola-1_0_1"
      (rectangle (start -31.75 26.67) (end 34.29 -29.21)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
  )
  (symbol "ESP32-S2-WROOM" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 45.72 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-S2-WROOM" (id 1) (at 0 -45.72 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-S2-WROOM" (id 2) (at 0 -48.26 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s2-wroom_esp32-s2-wroom-i_datasheet_en.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ESP32-S2-WROOM and ESP32-S2-WROOM-I" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S2-WROOM_0_0"
      (pin power_in line (at -35.56 -41.91 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ESP32-S2-WROOM_1_1"
      (rectangle (start -33.02 44.45) (end 34.29 -44.45)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "ESP32-S2-WROOM" (at 0 -39.37 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin power_in line (at -35.56 -34.29 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 17.78 0) (length 2.54)
        (name "GPIO7/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 15.24 0) (length 2.54)
        (name "GPIO8/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 12.7 0) (length 2.54)
        (name "GPIO9/ADC1_CH8" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 10.16 0) (length 2.54)
        (name "GPIO10/ADC1_CH9" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 7.62 0) (length 2.54)
        (name "GPIO11/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 5.08 0) (length 2.54)
        (name "GPIO12/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 2.54 0) (length 2.54)
        (name "GPIO13/ADC2_CH2" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 0 0) (length 2.54)
        (name "GPIO14/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 -10.16 0) (length 2.54)
        (name "GPIO15/ADC2_CH4/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 -16.51 0) (length 2.54)
        (name "GPIO16/ADC2_CH5/XTAL_32K_N" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -27.94 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -31.75 180) (length 2.54)
        (name "ADC2_CH7/DAC_2/GPIO17" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -29.21 180) (length 2.54)
        (name "ADC2_CH6/DAC_1/GPIO18" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -2.54 180) (length 2.54)
        (name "USB_D-/ADC2_CH8/GPIO19" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 0 180) (length 2.54)
        (name "USB_D+/ADC2_CH9/GPIO20" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 5.08 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 7.62 180) (length 2.54)
        (name "SPI_CS1/GPIO26" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -36.83 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 20.32 180) (length 2.54)
        (name "GPIO33" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 22.86 180) (length 2.54)
        (name "GPIO34" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 25.4 180) (length 2.54)
        (name "GPIO35" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -24.13 180) (length 2.54)
        (name "GPIO0/BOOT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 27.94 180) (length 2.54)
        (name "GPIO36" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 30.48 180) (length 2.54)
        (name "GPIO37" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 33.02 180) (length 2.54)
        (name "GPIO38" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -15.24 180) (length 2.54)
        (name "MTCK/JTAG/GPIO39" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -12.7 180) (length 2.54)
        (name "MTDO/JTAG/GPIO40" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -10.16 180) (length 2.54)
        (name "MTDI/JTAG/GPIO41" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -7.62 180) (length 2.54)
        (name "MTMS/JTAG/GPIO42" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 38.1 180) (length 2.54)
        (name "GPIO43/U0TXD/PROG" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 40.64 180) (length 2.54)
        (name "GPIO44/U0RXD/PROG" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -21.59 180) (length 2.54)
        (name "GPIO45" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 33.02 0) (length 2.54)
        (name "GPIO1/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 36.83 15.24 180) (length 2.54)
        (name "GPIO46" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -35.56 40.64 0) (length 2.54)
        (name "CHIP/PU/RESET" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -39.37 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 30.48 0) (length 2.54)
        (name "GPIO2/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 27.94 0) (length 2.54)
        (name "GPIO3/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 25.4 0) (length 2.54)
        (name "GPIO4/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 22.86 0) (length 2.54)
        (name "GPIO5/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 20.32 0) (length 2.54)
        (name "GPIO6/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-S2-WROVER" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 45.72 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-S2-WROVER" (id 1) (at 0 -45.72 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-S2-WROVER" (id 2) (at 0 -48.26 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s2-wroom_esp32-s2-wroom-i_datasheet_en.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S2-WROVER_0_0"
      (rectangle (start -33.02 44.45) (end 34.29 -44.45)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "ESP32-S2-WROVER" (at 0 -39.37 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin power_in line (at -35.56 -34.29 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 17.78 0) (length 2.54)
        (name "GPIO7/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 15.24 0) (length 2.54)
        (name "GPIO8/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 12.7 0) (length 2.54)
        (name "GPIO9/ADC1_CH8" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 10.16 0) (length 2.54)
        (name "GPIO10/ADC1_CH9" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 7.62 0) (length 2.54)
        (name "GPIO11/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 5.08 0) (length 2.54)
        (name "GPIO12/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 2.54 0) (length 2.54)
        (name "GPIO13/ADC2_CH2" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 0 0) (length 2.54)
        (name "GPIO14/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 -10.16 0) (length 2.54)
        (name "GPIO15/ADC2_CH4/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 -16.51 0) (length 2.54)
        (name "GPIO16/ADC2_CH5/XTAL_32K_N" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -27.94 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -31.75 180) (length 2.54)
        (name "ADC2_CH7/DAC_2/GPIO17" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -29.21 180) (length 2.54)
        (name "ADC2_CH6/DAC_1/GPIO18" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -2.54 180) (length 2.54)
        (name "USB_D-/ADC2_CH8/GPIO19" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 0 180) (length 2.54)
        (name "USB_D+/ADC2_CH9/GPIO20" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 5.08 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 7.62 180) (length 2.54)
        (name "SPI_CS1/GPIO26" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -36.83 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 20.32 180) (length 2.54)
        (name "GPIO33" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 22.86 180) (length 2.54)
        (name "GPIO34" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 25.4 180) (length 2.54)
        (name "GPIO35" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -24.13 180) (length 2.54)
        (name "GPIO0/BOOT" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 27.94 180) (length 2.54)
        (name "GPIO36" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 30.48 180) (length 2.54)
        (name "GPIO37" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 33.02 180) (length 2.54)
        (name "GPIO38" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -15.24 180) (length 2.54)
        (name "MTCK/JTAG/GPIO39" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -12.7 180) (length 2.54)
        (name "MTDO/JTAG/GPIO40" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -10.16 180) (length 2.54)
        (name "MTDI/JTAG/GPIO41" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -7.62 180) (length 2.54)
        (name "MTMS/JTAG/GPIO42" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 38.1 180) (length 2.54)
        (name "GPIO43/U0TXD/PROG" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 40.64 180) (length 2.54)
        (name "GPIO44/U0RXD/PROG" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 36.83 -21.59 180) (length 2.54)
        (name "GPIO45" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 33.02 0) (length 2.54)
        (name "GPIO1/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 36.83 15.24 180) (length 2.54)
        (name "GPIO46" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -35.56 40.64 0) (length 2.54)
        (name "CHIP/PU/RESET" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -39.37 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -35.56 -41.91 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 30.48 0) (length 2.54)
        (name "GPIO2/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 27.94 0) (length 2.54)
        (name "GPIO3/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 25.4 0) (length 2.54)
        (name "GPIO4/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 22.86 0) (length 2.54)
        (name "GPIO5/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -35.56 20.32 0) (length 2.54)
        (name "GPIO6/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-S3" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 46.99 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-S3" (id 1) (at 0 -43.18 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm" (id 2) (at 0 -45.72 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at -8.89 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S3_0_0"
      (text "ESP32-S3" (at 1.27 0 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin bidirectional line (at 30.48 -8.89 180) (length 2.54)
        (name "SPICLK_N/GPIO48" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -11.43 180) (length 2.54)
        (name "SPICLK_P/GPIO47" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ESP32-S3_0_1"
      (rectangle (start -29.21 45.72) (end 27.94 -41.91)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32-S3_1_1"
      (pin bidirectional line (at -31.75 43.18 0) (length 2.54)
        (name "LNA_IN/RF" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 24.13 0) (length 2.54)
        (name "GPIO5/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 21.59 0) (length 2.54)
        (name "GPIO6/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 19.05 0) (length 2.54)
        (name "GPIO7/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 16.51 0) (length 2.54)
        (name "GPIO8/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 13.97 0) (length 2.54)
        (name "GPIO9/ADC1_CH8" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 11.43 0) (length 2.54)
        (name "GPIO10/ADC1_CH9" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 8.89 0) (length 2.54)
        (name "GPIO11/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 6.35 0) (length 2.54)
        (name "GPIO12/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 3.81 0) (length 2.54)
        (name "GPIO13/ADC2_CH2" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 1.27 0) (length 2.54)
        (name "GPIO14/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -31.75 -31.75 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -31.75 -36.83 0) (length 2.54)
        (name "VDD3P3_RTC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at 30.48 -20.32 180) (length 2.54)
        (name "GPIO15/ADC2_CH4/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin output clock (at 30.48 -24.13 180) (length 2.54)
        (name "GPIO16/ADC2_CH5/XTAL_32K_N" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 34.29 180) (length 2.54)
        (name "GPIO17/ADC2_CH6/DAC_2" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 36.83 180) (length 2.54)
        (name "GPIO18/ADC2_CH7/DAC_1" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 43.18 180) (length 2.54)
        (name "GPIO19/USB_D-/ADC2_CH8" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 40.64 180) (length 2.54)
        (name "GPIO20/USB_D+/ADC2_CH9" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 31.75 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 29.21 180) (length 2.54)
        (name "SPI_CS1/GPIO26" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 30.48 -15.24 180) (length 2.54)
        (name "VDD_SPI" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -31.75 -34.29 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 26.67 180) (length 2.54)
        (name "SPIHD/GPIO27" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 24.13 180) (length 2.54)
        (name "SPIWP/GPIO28" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 21.59 180) (length 2.54)
        (name "SPICS0/GPIO29" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 19.05 180) (length 2.54)
        (name "SPICLK/GPIO30" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 16.51 180) (length 2.54)
        (name "SPIQ/GPIO31" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 13.97 180) (length 2.54)
        (name "SPID/GPIO32" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 11.43 180) (length 2.54)
        (name "GPIO33" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 8.89 180) (length 2.54)
        (name "GPIO34" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -31.75 39.37 0) (length 2.54)
        (name "CHIP_PU/RESET" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 6.35 180) (length 2.54)
        (name "GPIO35" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 3.81 180) (length 2.54)
        (name "GPIO36" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 1.27 180) (length 2.54)
        (name "GPIO37" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -1.27 180) (length 2.54)
        (name "GPIO38" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 -12.7 0) (length 2.54)
        (name "MTCK/JTAG/GPIO39" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 -15.24 0) (length 2.54)
        (name "MTDO/JTAG/GPIO40" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -31.75 -39.37 0) (length 2.54)
        (name "VDD3P3_CPU" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 -17.78 0) (length 2.54)
        (name "MTDI/JTAG/GPIO41" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 -20.32 0) (length 2.54)
        (name "MTMS/JTAG/GPIO42" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 -7.62 0) (length 2.54)
        (name "U0TXD/PROG/GPIO43" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 -5.08 0) (length 2.54)
        (name "GPIO0/BOOT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 -10.16 0) (length 2.54)
        (name "U0RXD/PROG/GPIO44" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -3.81 180) (length 2.54)
        (name "GPIO45" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -6.35 180) (length 2.54)
        (name "GPIO46" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at 30.48 -29.21 180) (length 2.54)
        (name "XTAL_N" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin output clock (at 30.48 -33.02 180) (length 2.54)
        (name "XTAL_P" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -31.75 -26.67 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -31.75 -29.21 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 30.48 -39.37 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 34.29 0) (length 2.54)
        (name "GPIO1/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 31.75 0) (length 2.54)
        (name "GPIO2/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 29.21 0) (length 2.54)
        (name "GPIO3/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 26.67 0) (length 2.54)
        (name "GPIO4/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-S3-DevKitC" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -2.54 30.48 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-S3-DevKitC" (id 1) (at 1.27 -33.02 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-S3-DevKitC" (id 2) (at 1.27 -35.56 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at -59.69 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S3-DevKitC_0_0"
      (pin bidirectional line (at -25.4 -7.62 0) (length 2.54)
        (name "GPIO46" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -20.32 0) (length 2.54)
        (name "GPIO13/ADC2_CH2" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -25.4 22.86 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 12.7 180) (length 2.54)
        (name "GPIO42/MTMS" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 15.24 180) (length 2.54)
        (name "GPIO2/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 17.78 180) (length 2.54)
        (name "GPIO1/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 20.32 180) (length 2.54)
        (name "GPIO44/U0RXD" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 22.86 180) (length 2.54)
        (name "GPIO43/U0TXD" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 25.4 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ESP32-S3-DevKitC_0_1"
      (rectangle (start 22.86 -31.75) (end -22.86 29.21)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32-S3-DevKitC_1_1"
      (pin power_in line (at -25.4 25.4 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 2.54 0) (length 2.54)
        (name "GPIO17/ADC2_CH6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 0 0) (length 2.54)
        (name "GPIO18/ADC2_CH7" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -2.54 0) (length 2.54)
        (name "GPIO8/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -5.08 0) (length 2.54)
        (name "GPIO3/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -10.16 0) (length 2.54)
        (name "GPIO9/ADC1_CH8" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -12.7 0) (length 2.54)
        (name "GPIO10/ADC1_CH9" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -15.24 0) (length 2.54)
        (name "GPIO11/ADC2_CH0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -17.78 0) (length 2.54)
        (name "GPIO12/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -22.86 0) (length 2.54)
        (name "GPIO14/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -25.4 -25.4 0) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -25.4 -27.94 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -27.94 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.4 -25.4 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -22.86 180) (length 2.54)
        (name "GPIO19/USB_D-" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -20.32 180) (length 2.54)
        (name "GPIO20/USB_D+" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -17.78 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -15.24 180) (length 2.54)
        (name "GPIO47" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -12.7 180) (length 2.54)
        (name "GPIO48" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -25.4 20.32 0) (length 2.54)
        (name "CHIP_PU" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -10.16 180) (length 2.54)
        (name "GPIO45" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -7.62 180) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -5.08 180) (length 2.54)
        (name "GPIO35" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -2.54 180) (length 2.54)
        (name "GPIO36" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 0 180) (length 2.54)
        (name "GPIO37" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 2.54 180) (length 2.54)
        (name "GPIO38" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 5.08 180) (length 2.54)
        (name "GPIO39/MTCK" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 7.62 180) (length 2.54)
        (name "GPIO40/MTDO" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 10.16 180) (length 2.54)
        (name "GPIO41/MTDI" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 17.78 0) (length 2.54)
        (name "GPIO4/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 15.24 0) (length 2.54)
        (name "GPIO5/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 12.7 0) (length 2.54)
        (name "GPIO6/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 10.16 0) (length 2.54)
        (name "GPIO7/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 7.62 0) (length 2.54)
        (name "GPIO15/ADC2_CH4/32K_P" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 5.08 0) (length 2.54)
        (name "GPIO16/ADC2_CH5/32K_N" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-S3-MINI-1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 35.56 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-S3-MINI-1" (id 1) (at 0 -39.37 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-S3-MINI-1" (id 2) (at 0 -41.91 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S3-MINI-1_0_0"
      (rectangle (start -57.15 34.29) (end 55.88 -38.1)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "ESP32-S3-MINI-1" (at 0 -31.75 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin power_in line (at 58.42 -24.13 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 10.16 0) (length 2.54)
        (name "GPIO6/TOUCH6/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 7.62 0) (length 2.54)
        (name "GPIO7/TOUCH7/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 5.08 0) (length 2.54)
        (name "GPIO8/TOUCH8/ADC1_CH7/SUBSPICS1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 2.54 0) (length 2.54)
        (name "GPIO9/TOUCH9/ADC1_CH8/FSPIHD/SUBSPIHD" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 0 0) (length 2.54)
        (name "GPIO10/TOUCH10/ADC1_CH9/FSPICS0/FSPIIO4/SUBSPICS0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -2.54 0) (length 2.54)
        (name "GPIO11/TOUCH11/ADC2_CH0/FSPICS0/FSPIIO4/SUBSPICS0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -5.08 0) (length 2.54)
        (name "GPIO12/TOUCH11/ADC2_CH0/FSPICS0/FSPIIO4/SUBSPICS0" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -7.62 0) (length 2.54)
        (name "GPIO13/TOUCH13/ADC2_CH2/FSPIQ/FSPIIO7/SUBSPIQ" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -10.16 0) (length 2.54)
        (name "GPIO14/TOUCH14/ADC2_CH3/FSPIWP/FSPIDQS/SUBSPIWP" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -12.7 0) (length 2.54)
        (name "GPIO15/U0RTS/ADC2_CH4/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 58.42 -26.67 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -15.24 0) (length 2.54)
        (name "GPIO16/U0CTS/ADC2_CH5/XTAL_32K_NH5" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -17.78 0) (length 2.54)
        (name "GPIO17/U1TXD/ADC2_CH6" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -20.32 0) (length 2.54)
        (name "GPIO18/U1RXD/ADC2_CH7/CLK_OUT3" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 29.21 180) (length 2.54)
        (name "GPIO19/U1RTS/ADC2_CH8/CLK_OUT2/USB_D-" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 31.75 180) (length 2.54)
        (name "GPIO20/U1CTS/ADC2_CH9/CLK_OUT1/USB_D+" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 20.32 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 17.78 180) (length 2.54)
        (name "GPIO26" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 7.62 180) (length 2.54)
        (name "GPIO47/SPICLK_P/SUBSPICLK_P_DIFF" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 5.08 180) (length 2.54)
        (name "SPIIO4/GPIO33/FSPIHD/SUBSPIHD" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 2.54 180) (length 2.54)
        (name "SPIIO5/GPIO34/FSPICS0/SUBSPICS0" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -59.69 -29.21 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 10.16 180) (length 2.54)
        (name "GPIO48/SPICLK_N/SUBSPICLK_N_DIFF" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 0 180) (length 2.54)
        (name "SPIIO6/GPIO35/FSPID/SUBSPID" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -2.54 180) (length 2.54)
        (name "SPIIO7/GPIO36/FSPICLK/SUBSPICLK" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -5.08 180) (length 2.54)
        (name "SPIDQS/GPIO37/FSPIQ/SUBSPIQ" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -7.62 180) (length 2.54)
        (name "GPIO38/FSPIWP/SUBSPIWP" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -11.43 180) (length 2.54)
        (name "MTCK/GPIO39/CLK_OUT3/SUBSPICS1" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -13.97 180) (length 2.54)
        (name "MTDO/GPIO40/CLK_OUT2" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -16.51 180) (length 2.54)
        (name "MTDI/GPIO41/CLK_OUT1" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -19.05 180) (length 2.54)
        (name "MTMS/GPIO42" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 25.4 180) (length 2.54)
        (name "U0TXD/GPIO43/CLK_OUT1" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 29.21 0) (length 2.54)
        (name "GPIO0/BOOT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 22.86 180) (length 2.54)
        (name "U0RXD/GPIO44/CLK_OUT2" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 15.24 180) (length 2.54)
        (name "GPIO45" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 58.42 -29.21 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 58.42 -31.75 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 12.7 180) (length 2.54)
        (name "GPIO46" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -59.69 26.67 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 58.42 -34.29 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 22.86 0) (length 2.54)
        (name "GPIO1/TOUCH1/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 20.32 0) (length 2.54)
        (name "GPIO2/TOUCH2/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 17.78 0) (length 2.54)
        (name "GPIO3/TOUCH3/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 15.24 0) (length 2.54)
        (name "GPIO4/TOUCH4/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 12.7 0) (length 2.54)
        (name "GPIO5/TOUCH5/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-S3-WROOM-1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 35.56 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-S3-WROOM-1" (id 1) (at 0 -36.83 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-S3-WROOM-1" (id 2) (at 0 -39.37 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-S3-WROOM-1_0_0"
      (rectangle (start -57.15 34.29) (end 55.88 -35.56)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "ESP32-S3-WROOM-1" (at 0 -31.75 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin power_in line (at 58.42 -27.94 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -17.78 0) (length 2.54)
        (name "GPIO17/U1TXD/ADC2_CH6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -20.32 0) (length 2.54)
        (name "GPIO18/U1RXD/ADC2_CH7/CLK_OUT3" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 5.08 0) (length 2.54)
        (name "GPIO8/TOUCH8/ADC1_CH7/SUBSPICS1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 29.21 180) (length 2.54)
        (name "GPIO19/U1RTS/ADC2_CH8/CLK_OUT2/USB_D-" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 31.75 180) (length 2.54)
        (name "GPIO20/U1CTS/ADC2_CH9/CLK_OUT1/USB_D+" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 17.78 0) (length 2.54)
        (name "GPIO3/TOUCH3/ADC1_CH2" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 8.89 180) (length 2.54)
        (name "GPIO46" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 2.54 0) (length 2.54)
        (name "GPIO9/TOUCH9/ADC1_CH8/FSPIHD/SUBSPIHD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 0 0) (length 2.54)
        (name "GPIO10/TOUCH10/ADC1_CH9/FSPICS0/FSPIIO4/SUBSPICS0" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -2.54 0) (length 2.54)
        (name "GPIO11/TOUCH11/ADC2_CH0/FSPICS0/FSPIIO4/SUBSPICS0" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -59.69 -30.48 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -5.08 0) (length 2.54)
        (name "GPIO12/TOUCH11/ADC2_CH0/FSPICS0/FSPIIO4/SUBSPICS0" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -7.62 0) (length 2.54)
        (name "GPIO13/TOUCH13/ADC2_CH2/FSPIQ/FSPIIO7/SUBSPIQ" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -10.16 0) (length 2.54)
        (name "GPIO14/TOUCH14/ADC2_CH3/FSPIWP/FSPIDQS/SUBSPIWP" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 13.97 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 3.81 180) (length 2.54)
        (name "GPIO47/SPICLK_P/SUBSPICLK_P_DIFF" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 6.35 180) (length 2.54)
        (name "GPIO48/SPICLK_N/SUBSPICLK_N_DIFF" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 11.43 180) (length 2.54)
        (name "GPIO45" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 29.21 0) (length 2.54)
        (name "GPIO0/BOOT" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -1.27 180) (length 2.54)
        (name "SPIIO6/GPIO35/FSPID/SUBSPID" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -3.81 180) (length 2.54)
        (name "SPIIO7/GPIO36/FSPICLK/SUBSPICLK" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -59.69 26.67 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -6.35 180) (length 2.54)
        (name "SPIDQS/GPIO37/FSPIQ/SUBSPIQ" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -8.89 180) (length 2.54)
        (name "GPIO38/FSPIWP/SUBSPIWP" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -13.97 180) (length 2.54)
        (name "MTCK/GPIO39/CLK_OUT3/SUBSPICS1" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -16.51 180) (length 2.54)
        (name "MTDO/GPIO40/CLK_OUT2" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -19.05 180) (length 2.54)
        (name "MTDI/GPIO41/CLK_OUT1" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 -21.59 180) (length 2.54)
        (name "MTMS/GPIO42" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 19.05 180) (length 2.54)
        (name "U0RXD/GPIO44/CLK_OUT2" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 58.42 21.59 180) (length 2.54)
        (name "U0TXD/GPIO43/CLK_OUT1" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 20.32 0) (length 2.54)
        (name "GPIO2/TOUCH2/ADC1_CH1" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 22.86 0) (length 2.54)
        (name "GPIO1/TOUCH1/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 15.24 0) (length 2.54)
        (name "GPIO4/TOUCH4/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 58.42 -30.48 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 58.42 -33.02 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 12.7 0) (length 2.54)
        (name "GPIO5/TOUCH5/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 10.16 0) (length 2.54)
        (name "GPIO6/TOUCH6/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 7.62 0) (length 2.54)
        (name "GPIO7/TOUCH7/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -12.7 0) (length 2.54)
        (name "GPIO15/U0RTS/ADC2_CH4/XTAL_32K_P" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -59.69 -15.24 0) (length 2.54)
        (name "GPIO16/U0CTS/ADC2_CH5/XTAL_32K_NH5" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-WROOM-E" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 43.18 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-WROOM-E" (id 1) (at 0 -41.91 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-WROOM-32E" (id 2) (at 0 -44.45 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf" (id 3) (at 10.16 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "ESP32" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ESP32-WROVER-E and ESP32-WROVER-IE are two powerful, generic WiFi-BT-BLE MCU modules that target a wide variety of applications, ranging from low-power sensor networks to the most demanding tasks, such as voice encoding, music streaming and MP3 decoding. ESP32-WROVER-E comes with a PCB antenna, and ESP32-WROVER-IE with an IPEX antenna. They both featurea 4 MB external SPI flash and an additional 8 MB SPI Pseudo static RAM (PSRAM)." (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-WROOM-E_0_1"
      (rectangle (start 33.02 41.91) (end -31.75 -40.64)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32-WROOM-E_1_1"
      (text "ESP32-­WROOM­" (at 1.27 36.83 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin power_in line (at 35.56 -33.02 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 0 180) (length 2.54)
        (name "DAC_1/ADC2_CH8/GPIO25" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 -2.54 180) (length 2.54)
        (name "DAC_2/ADC2_CH9/GPIO26" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 -5.08 180) (length 2.54)
        (name "ADC2_CH7/GPIO27" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -19.05 0) (length 2.54)
        (name "MTMS/GPIO14/ADC2_CH6" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -21.59 0) (length 2.54)
        (name "MTDI/GPIO12/ADC2_CH5" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 35.56 -35.56 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -24.13 0) (length 2.54)
        (name "MTCK/GPIO13/ADC2_CH4" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -17.78 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -20.32 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -22.86 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -34.29 -35.56 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -25.4 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -12.7 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -15.24 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -26.67 0) (length 2.54)
        (name "MTDO/GPIO15/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 25.4 180) (length 2.54)
        (name "ADC2_CH2/GPIO2" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 13.97 0) (length 2.54)
        (name "GPIO0/BOOT/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 22.86 180) (length 2.54)
        (name "ADC2_CH0/GPIO4" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 17.78 180) (length 2.54)
        (name "GPIO16" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 15.24 180) (length 2.54)
        (name "GPIO17" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 20.32 180) (length 2.54)
        (name "GPIO5" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -34.29 25.4 0) (length 2.54)
        (name "EN/CHIP_PU" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 12.7 180) (length 2.54)
        (name "GPIO18" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 10.16 180) (length 2.54)
        (name "GPIO19" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -27.94 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 7.62 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 19.05 0) (length 2.54)
        (name "U0RXD/GPIO3" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 16.51 0) (length 2.54)
        (name "U0TXD/GPIO1" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 5.08 180) (length 2.54)
        (name "GPIO22" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 2.54 180) (length 2.54)
        (name "GPIO23" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 35.56 -38.1 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -34.29 8.89 0) (length 2.54)
        (name "SENSOR_VP/GPIO36/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -34.29 6.35 0) (length 2.54)
        (name "SENSOR_VN/GPIO39/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -34.29 3.81 0) (length 2.54)
        (name "GPIO34/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -34.29 1.27 0) (length 2.54)
        (name "GPIO35/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -6.35 0) (length 2.54)
        (name "32K_XP/GPIO32/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -11.43 0) (length 2.54)
        (name "32K_XN/GPIO33/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP32-WROVER-E" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 43.18 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP32-WROVER-E" (id 1) (at 0 -41.91 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Espressif:ESP32-WROVER-E" (id 2) (at 0 -44.45 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wrover-e_esp32-wrover-ie_datasheet_en.pdf" (id 3) (at 10.16 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "ESP32" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ESP32-WROVER-E and ESP32-WROVER-IE are two powerful, generic WiFi-BT-BLE MCU modules that target a wide variety of applications, ranging from low-power sensor networks to the most demanding tasks, such as voice encoding, music streaming and MP3 decoding. ESP32-WROVER-E comes with a PCB antenna, and ESP32-WROVER-IE with an IPEX antenna. They both featurea 4 MB external SPI flash and an additional 8 MB SPI Pseudo static RAM (PSRAM)." (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP32-WROVER-E_0_1"
      (rectangle (start 33.02 41.91) (end -31.75 -40.64)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "ESP32-WROVER-E_1_1"
      (text "ESP32-­WROVER" (at 1.27 36.83 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin power_in line (at 35.56 -33.02 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 0 180) (length 2.54)
        (name "DAC_1/ADC2_CH8/GPIO25" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 -2.54 180) (length 2.54)
        (name "DAC_2/ADC2_CH9/GPIO26" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 -5.08 180) (length 2.54)
        (name "ADC2_CH7/GPIO27" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -19.05 0) (length 2.54)
        (name "MTMS/GPIO14/ADC2_CH6" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -21.59 0) (length 2.54)
        (name "MTDI/GPIO12/ADC2_CH5" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 35.56 -35.56 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -24.13 0) (length 2.54)
        (name "MTCK/GPIO13/ADC2_CH4" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -17.78 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -20.32 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -22.86 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -34.29 -35.56 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -25.4 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -12.7 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -15.24 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -26.67 0) (length 2.54)
        (name "MTDO/GPIO15/ADC2_CH3" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 25.4 180) (length 2.54)
        (name "ADC2_CH2/GPIO2" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 13.97 0) (length 2.54)
        (name "GPIO0/BOOT/ADC2_CH1" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 22.86 180) (length 2.54)
        (name "ADC2_CH0/GPIO4" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 17.78 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 15.24 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 20.32 180) (length 2.54)
        (name "GPIO5" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -34.29 25.4 0) (length 2.54)
        (name "EN/CHIP_PU" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 12.7 180) (length 2.54)
        (name "GPIO18" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 10.16 180) (length 2.54)
        (name "GPIO19" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 35.56 -27.94 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 7.62 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 19.05 0) (length 2.54)
        (name "U0RXD/GPIO3" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 16.51 0) (length 2.54)
        (name "U0TXD/GPIO1" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 5.08 180) (length 2.54)
        (name "GPIO22" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 35.56 2.54 180) (length 2.54)
        (name "GPIO23" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 35.56 -38.1 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -34.29 8.89 0) (length 2.54)
        (name "SENSOR_VP/GPIO36/ADC1_CH0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -34.29 6.35 0) (length 2.54)
        (name "SENSOR_VN/GPIO39/ADC1_CH3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -34.29 3.81 0) (length 2.54)
        (name "GPIO34/ADC1_CH6" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -34.29 1.27 0) (length 2.54)
        (name "GPIO35/ADC1_CH7" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -6.35 0) (length 2.54)
        (name "32K_XP/GPIO32/ADC1_CH4" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -11.43 0) (length 2.54)
        (name "32K_XN/GPIO33/ADC1_CH5" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP8266" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP8266" (id 1) (at 0 -27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm" (id 2) (at 0 -30.48 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/0a-esp8266ex_datasheet_en.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Espressif’s ESP8266EX delivers highly integrated Wi-Fi SoC solution to meet users’ continuous demands for efficient power usage, compact design and reliable performance in the Internet of Things industry." (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP8266_1_1"
      (rectangle (start -25.4 30.48) (end 25.4 -26.67)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "ESP8266" (at 0 15.24 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin bidirectional line (at -27.94 -11.43 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 6.35 0) (length 2.54)
        (name "MTDI/GPIO12" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -21.59 0) (length 2.54)
        (name "VDDPST" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 3.81 0) (length 2.54)
        (name "MTCK/GPIO13" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 1.27 0) (length 2.54)
        (name "MTDO/GPIO15" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -12.7 180) (length 2.54)
        (name "GPIO2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -10.16 180) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -7.62 180) (length 2.54)
        (name "GPIO4" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -24.13 0) (length 2.54)
        (name "VDDPST" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -5.08 180) (length 2.54)
        (name "SDIO_DATA_2/GPIO9" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -2.54 180) (length 2.54)
        (name "SDIO_DATA_3/GPIO10" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 27.94 0) (length 2.54)
        (name "LNA" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 0 180) (length 2.54)
        (name "SDIO_CMD/GPIO11" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 2.54 180) (length 2.54)
        (name "SDIO_CLK/GPIO6" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 5.08 180) (length 2.54)
        (name "SDIO_DATA_0/GPIO7" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 7.62 180) (length 2.54)
        (name "SDIO_DATA_1/GPIO8" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 10.16 180) (length 2.54)
        (name "GPIO5" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 12.7 180) (length 2.54)
        (name "U0RXD/GPIO3" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 15.24 180) (length 2.54)
        (name "U0TXD/GPIO1" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 21.59 180) (length 2.54)
        (name "XTAL_OUT" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 27.94 180) (length 2.54)
        (name "XTAL_IN" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -27.94 -16.51 0) (length 2.54)
        (name "VDDD" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -27.94 -19.05 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -27.94 -13.97 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -6.35 0) (length 2.54)
        (name "RES12K" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -3.81 0) (length 2.54)
        (name "EXT_RSTB" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 -24.13 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -27.94 17.78 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -27.94 15.24 0) (length 2.54)
        (name "VDD_RTC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -17.78 180) (length 2.54)
        (name "TOUT/ADC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -27.94 22.86 0) (length 2.54)
        (name "CHIP_EN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -15.24 180) (length 2.54)
        (name "XPD_DCDC/GPIO16" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 8.89 0) (length 2.54)
        (name "MTMS/GPIO14" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ESP8285" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ESP8285" (id 1) (at 0 -27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm" (id 2) (at 0 -30.48 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/0a-esp8285_datasheet_en.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Espressif's ESP8285 delivers highly integrated Wi-Fi SoC solution to meet users' continuous demands for efficient power usage, compact design and reliable performance in the Internet of Things industry." (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ESP8285_1_1"
      (rectangle (start -25.4 30.48) (end 25.4 -26.67)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (text "ESP8285" (at 0 15.24 0)
        (effects (font (size 2.54 2.54)))
      )
      (pin bidirectional line (at -27.94 -11.43 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 6.35 0) (length 2.54)
        (name "MTDI/GPIO12" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -21.59 0) (length 2.54)
        (name "VDDPST" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 3.81 0) (length 2.54)
        (name "MTCK/GPIO13" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 1.27 0) (length 2.54)
        (name "MTDO/GPIO15" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -12.7 180) (length 2.54)
        (name "GPIO2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -10.16 180) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -7.62 180) (length 2.54)
        (name "GPIO4" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -24.13 0) (length 2.54)
        (name "VDDPST" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -5.08 180) (length 2.54)
        (name "SDIO_DATA_2/GPIO9" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -2.54 180) (length 2.54)
        (name "SDIO_DATA_3/GPIO10" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 27.94 0) (length 2.54)
        (name "LNA" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 0 180) (length 2.54)
        (name "SDIO_CMD/GPIO11" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 2.54 180) (length 2.54)
        (name "SDIO_CLK/GPIO6" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 5.08 180) (length 2.54)
        (name "SDIO_DATA_0/GPIO7" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 7.62 180) (length 2.54)
        (name "SDIO_DATA_1/GPIO8" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 10.16 180) (length 2.54)
        (name "GPIO5" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 12.7 180) (length 2.54)
        (name "U0RXD/GPIO3" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 15.24 180) (length 2.54)
        (name "U0TXD/GPIO1" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 21.59 180) (length 2.54)
        (name "XTAL_OUT" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 27.94 180) (length 2.54)
        (name "XTAL_IN" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -27.94 -16.51 0) (length 2.54)
        (name "VDDD" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -27.94 -19.05 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -27.94 -13.97 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -6.35 0) (length 2.54)
        (name "RES12K" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -27.94 -3.81 0) (length 2.54)
        (name "EXT_RSTB" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 27.94 -24.13 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -27.94 17.78 0) (length 2.54)
        (name "VDD3P3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -27.94 15.24 0) (length 2.54)
        (name "VDD_RTC" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -17.78 180) (length 2.54)
        (name "TOUT/ADC" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -27.94 22.86 0) (length 2.54)
        (name "CHIP_EN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -15.24 180) (length 2.54)
        (name "XPD_DCDC/GPIO16" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -27.94 8.89 0) (length 2.54)
        (name "MTMS/GPIO14" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
