#============================================================
# Build by Terasic System Builder
#============================================================

set_global_assignment -name DEVICE 5CSEBA6U23I7
set_global_assignment -name FAMILY "Cyclone V"
set_global_assignment -name TOP_LEVEL_ENTITY DE10_nano_zpu
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 10.1
set_global_assignment -name LAST_QUARTUS_VERSION "17.1.1 Standard Edition"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "16:22:00 FEBRUARY 21,2011"
set_global_assignment -name DEVICE_FILTER_PACKAGE UFBGA
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 672
set_global_assignment -name DEVICE_FILTER_SPEED_GRADE 7
set_global_assignment -name RESERVE_FLASH_NCE_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name RESERVE_DATA0_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name RESERVE_DATA1_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name RESERVE_DCLK_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name GENERATE_RBF_FILE ON


#============================================================
# UART
#============================================================
#set_location_assignment PIN_AA13 -to UART_TX_0
#set_location_assignment PIN_AA11 -to UART_RX_0
#set_location_assignment PIN_Y11 -to UART_TX_1
#set_location_assignment PIN_AA26 -to UART_RX_1
set_location_assignment PIN_Y15 -to UART_TX_0
set_location_assignment PIN_AA15 -to UART_RX_0
set_location_assignment PIN_AG28 -to UART_TX_1
set_location_assignment PIN_AG26 -to UART_RX_1
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to UART_TX_0
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to UART_RX_0
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to UART_TX_1
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to UART_RX_1
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to UART_TX_0
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to UART_TX_1

#============================================================
# SD CARD
#============================================================
set_location_assignment PIN_AF25 -to SDCARD_MISO[0]
set_location_assignment PIN_AF27 -to SDCARD_MOSI[0]
set_location_assignment PIN_AH26 -to SDCARD_CLK[0]
set_location_assignment PIN_AF28 -to SDCARD_CS[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDCARD_MISO[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDCARD_MOSI[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDCARD_CLK[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDCARD_CS[0]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDCARD_MOSI[0]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDCARD_CLK[0]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDCARD_CS[0]

#============================================================
# CLOCK
#============================================================
#set_location_assignment PIN_R8 -to CLOCK_50
set_location_assignment PIN_V11 -to CLOCK_50
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to CLOCK_50

#============================================================
# LED
#============================================================
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LED[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LED[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LED[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LED[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LED[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LED[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LED[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LED[7]
set_location_assignment PIN_W15 -to LED[0]
set_location_assignment PIN_AA24 -to LED[1]
set_location_assignment PIN_V16 -to LED[2]
set_location_assignment PIN_V15 -to LED[3]
set_location_assignment PIN_AF26 -to LED[4]
set_location_assignment PIN_AE26 -to LED[5]
set_location_assignment PIN_Y16 -to LED[6]
set_location_assignment PIN_AA23 -to LED[7]

#============================================================
# KEY
#============================================================
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to KEY[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to KEY[1]
set_location_assignment PIN_AH17 -to KEY[0]
set_location_assignment PIN_AH16 -to KEY[1]

#============================================================
# SW
#============================================================
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[3]
set_location_assignment PIN_Y24 -to SW[0]
set_location_assignment PIN_W24 -to SW[1]
set_location_assignment PIN_W21 -to SW[2]
set_location_assignment PIN_W20 -to SW[3]

#============================================================
# SDIO
#============================================================
#set_location_assignment PIN_AF25 -to SDIO_DAT[0]
#set_location_assignment PIN_AF23 -to SDIO_DAT[1]
#set_location_assignment PIN_AD26 -to SDIO_DAT[2]
#set_location_assignment PIN_AF28 -to SDIO_DAT[3]
#set_location_assignment PIN_AF27 -to SDIO_CMD
#set_location_assignment PIN_AH26 -to SDIO_CLK
#set_location_assignment PIN_AH7 -to SDIO_CD
#set_location_assignment PIN_AF25 -to TDO
#set_location_assignment PIN_AF28 -to TCS
#set_location_assignment PIN_AF27 -to TDI
#set_location_assignment PIN_AH26 -to TCK

#set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDIO_*

#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to TDO
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to TDI
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to TCK
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to TCS
#set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to TDO
#set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to TCS
#set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to TDI

#============================================================
# SDRAM
#============================================================
#set_location_assignment PIN_M7 -to SDRAM_BA[0]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_BA[0]
#set_location_assignment PIN_M6 -to SDRAM_BA[1]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_BA[1]
#set_location_assignment PIN_R6 -to SDRAM_DQM[0]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQM[0]
#set_location_assignment PIN_T5 -to SDRAM_DQM[1]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQM[1]
#set_location_assignment PIN_L2 -to SDRAM_RAS_N
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_RAS_N
#set_location_assignment PIN_L1 -to SDRAM_CAS_N
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_CAS_N
#set_location_assignment PIN_L7 -to SDRAM_CKE
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_CKE
#set_location_assignment PIN_R4 -to SDRAM_CLK
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_CLK
#set_location_assignment PIN_C2 -to SDRAM_WE_N
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_WE_N
#set_location_assignment PIN_P6 -to SDRAM_CS_N
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_CS_N
#set_location_assignment PIN_G2 -to SDRAM_DQ[0]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[0]
#set_location_assignment PIN_G1 -to SDRAM_DQ[1]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[1]
#set_location_assignment PIN_L8 -to SDRAM_DQ[2]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[2]
#set_location_assignment PIN_K5 -to SDRAM_DQ[3]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[3]
#set_location_assignment PIN_K2 -to SDRAM_DQ[4]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[4]
#set_location_assignment PIN_J2 -to SDRAM_DQ[5]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[5]
#set_location_assignment PIN_J1 -to SDRAM_DQ[6]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[6]
#set_location_assignment PIN_R7 -to SDRAM_DQ[7]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[7]
#set_location_assignment PIN_T4 -to SDRAM_DQ[8]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[8]
#set_location_assignment PIN_T2 -to SDRAM_DQ[9]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[9]
#set_location_assignment PIN_T3 -to SDRAM_DQ[10]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[10]
#set_location_assignment PIN_R3 -to SDRAM_DQ[11]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[11]
#set_location_assignment PIN_R5 -to SDRAM_DQ[12]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[12]
#set_location_assignment PIN_P3 -to SDRAM_DQ[13]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[13]
#set_location_assignment PIN_N3 -to SDRAM_DQ[14]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[14]
#set_location_assignment PIN_K1 -to SDRAM_DQ[15]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_DQ[15]
#set_location_assignment PIN_P2 -to SDRAM_ADDR[0]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[0]
#set_location_assignment PIN_N5 -to SDRAM_ADDR[1]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[1]
#set_location_assignment PIN_N6 -to SDRAM_ADDR[2]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[2]
#set_location_assignment PIN_M8 -to SDRAM_ADDR[3]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[3]
#set_location_assignment PIN_P8 -to SDRAM_ADDR[4]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[4]
#set_location_assignment PIN_T7 -to SDRAM_ADDR[5]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[5]
#set_location_assignment PIN_N8 -to SDRAM_ADDR[6]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[6]
#set_location_assignment PIN_T6 -to SDRAM_ADDR[7]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[7]
#set_location_assignment PIN_R1 -to SDRAM_ADDR[8]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[8]
#set_location_assignment PIN_P1 -to SDRAM_ADDR[9]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[9]
#set_location_assignment PIN_N2 -to SDRAM_ADDR[10]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[10]
#set_location_assignment PIN_N1 -to SDRAM_ADDR[11]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[11]
#set_location_assignment PIN_L4 -to SDRAM_ADDR[12]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SDRAM_ADDR[12]

#============================================================
# EPCS
#============================================================
#set_location_assignment PIN_H2 -to EPCS_DATA0
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to EPCS_DATA0
#set_location_assignment PIN_H1 -to EPCS_DCLK
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to EPCS_DCLK
#set_location_assignment PIN_D2 -to EPCS_NCSO
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to EPCS_NCSO
#set_location_assignment PIN_C1 -to EPCS_ASDO
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to EPCS_ASDO

#============================================================
# Accelerometer and EEPROM
#============================================================
#set_location_assignment PIN_F2 -to I2C_SCLK
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to I2C_SCLK
#set_location_assignment PIN_F1 -to I2C_SDAT
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to I2C_SDAT
#set_location_assignment PIN_G5 -to G_SENSOR_CS_N
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to G_SENSOR_CS_N
#set_location_assignment PIN_M2 -to G_SENSOR_INT
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to G_SENSOR_INT

#============================================================
# ADC
#============================================================
#set_location_assignment PIN_A10 -to ADC_CS_N
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_CS_N
#set_location_assignment PIN_B10 -to ADC_SADDR
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_SADDR
#set_location_assignment PIN_B14 -to ADC_SCLK
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_SCLK
#set_location_assignment PIN_A9 -to ADC_SDAT
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_SDAT

#============================================================
# 2x13 GPIO Header
#============================================================
#set_location_assignment PIN_A14 -to GPIO_2[0]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[0]
#set_location_assignment PIN_B16 -to GPIO_2[1]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[1]
#set_location_assignment PIN_C14 -to GPIO_2[2]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[2]
#set_location_assignment PIN_C16 -to GPIO_2[3]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[3]
#set_location_assignment PIN_C15 -to GPIO_2[4]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[4]
#set_location_assignment PIN_D16 -to GPIO_2[5]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[5]
#set_location_assignment PIN_D15 -to GPIO_2[6]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[6]
#set_location_assignment PIN_D14 -to GPIO_2[7]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[7]
#set_location_assignment PIN_F15 -to GPIO_2[8]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[8]
#set_location_assignment PIN_F16 -to GPIO_2[9]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[9]
#set_location_assignment PIN_F14 -to GPIO_2[10]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[10]
#set_location_assignment PIN_G16 -to GPIO_2[11]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[11]
#set_location_assignment PIN_G15 -to GPIO_2[12]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2[12]
#set_location_assignment PIN_E15 -to GPIO_2_IN[0]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2_IN[0]
#set_location_assignment PIN_E16 -to GPIO_2_IN[1]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2_IN[1]
#set_location_assignment PIN_M16 -to GPIO_2_IN[2]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_2_IN[2]

#============================================================
# GPIO_0, GPIO_0 connect to GPIO Default
#============================================================
#set_location_assignment PIN_A8 -to GPIO_0_IN[0]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0_IN[0]
#set_location_assignment PIN_D3 -to GPIO_0[0]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[0]
#set_location_assignment PIN_B8 -to GPIO_0_IN[1]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0_IN[1]
#set_location_assignment PIN_C3 -to GPIO_0[1]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[1]
#set_location_assignment PIN_A2 -to GPIO_0[2]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[2]
#set_location_assignment PIN_A3 -to GPIO_0[3]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[3]
#set_location_assignment PIN_B3 -to GPIO_0[4]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[4]
#set_location_assignment PIN_B4 -to GPIO_0[5]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[5]
#set_location_assignment PIN_A4 -to GPIO_0[6]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[6]
#set_location_assignment PIN_B5 -to GPIO_0[7]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[7]
#set_location_assignment PIN_A5 -to GPIO_0[8]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[8]
#set_location_assignment PIN_D5 -to GPIO_0[9]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[9]
#set_location_assignment PIN_B6 -to GPIO_0[10]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[10]
#set_location_assignment PIN_A6 -to GPIO_0[11]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[11]
#set_location_assignment PIN_B7 -to GPIO_0[12]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[12]
#set_location_assignment PIN_D6 -to GPIO_0[13]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[13]
#set_location_assignment PIN_A7 -to GPIO_0[14]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[14]
#set_location_assignment PIN_C6 -to GPIO_0[15]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[15]
#set_location_assignment PIN_C8 -to GPIO_0[16]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[16]
#set_location_assignment PIN_E6 -to GPIO_0[17]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[17]
#set_location_assignment PIN_E7 -to GPIO_0[18]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[18]
#set_location_assignment PIN_D8 -to GPIO_0[19]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[19]
#set_location_assignment PIN_E8 -to GPIO_0[20]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[20]
#set_location_assignment PIN_F8 -to GPIO_0[21]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[21]
#set_location_assignment PIN_F9 -to GPIO_0[22]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[22]
#set_location_assignment PIN_E9 -to GPIO_0[23]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[23]
#set_location_assignment PIN_C9 -to GPIO_0[24]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[24]
#set_location_assignment PIN_D9 -to GPIO_0[25]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[25]
#set_location_assignment PIN_E11 -to GPIO_0[26]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[26]
#set_location_assignment PIN_E10 -to GPIO_0[27]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[27]
#set_location_assignment PIN_C11 -to GPIO_0[28]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[28]
#set_location_assignment PIN_B11 -to GPIO_0[29]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[29]
#set_location_assignment PIN_A12 -to GPIO_0[30]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[30]
#set_location_assignment PIN_D11 -to GPIO_0[31]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[31]
#set_location_assignment PIN_D12 -to GPIO_0[32]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[32]
#set_location_assignment PIN_B12 -to GPIO_0[33]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_0[33]

#============================================================
# GPIO_1, GPIO_1 connect to GPIO Default
#============================================================
#set_location_assignment PIN_T9 -to GPIO_1_IN[0]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1_IN[0]
#set_location_assignment PIN_F13 -to GPIO_1[0]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[0]
#set_location_assignment PIN_R9 -to GPIO_1_IN[1]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1_IN[1]
#set_location_assignment PIN_T15 -to GPIO_1[1]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[1]
#set_location_assignment PIN_T14 -to GPIO_1[2]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[2]
#set_location_assignment PIN_T13 -to GPIO_1[3]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[3]
#set_location_assignment PIN_R13 -to GPIO_1[4]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[4]
#set_location_assignment PIN_T12 -to GPIO_1[5]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[5]
#set_location_assignment PIN_R12 -to GPIO_1[6]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[6]
#set_location_assignment PIN_T11 -to GPIO_1[7]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[7]
#set_location_assignment PIN_T10 -to GPIO_1[8]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[8]
#set_location_assignment PIN_R11 -to GPIO_1[9]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[9]
#set_location_assignment PIN_P11 -to GPIO_1[10]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[10]
#set_location_assignment PIN_R10 -to GPIO_1[11]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[11]
#set_location_assignment PIN_N12 -to GPIO_1[12]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[12]
#set_location_assignment PIN_P9 -to GPIO_1[13]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[13]
#set_location_assignment PIN_N9 -to GPIO_1[14]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[14]
#set_location_assignment PIN_N11 -to GPIO_1[15]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[15]
#set_location_assignment PIN_L16 -to GPIO_1[16]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[16]
#set_location_assignment PIN_K16 -to GPIO_1[17]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[17]
#set_location_assignment PIN_R16 -to GPIO_1[18]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[18]
#set_location_assignment PIN_L15 -to GPIO_1[19]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[19]
#set_location_assignment PIN_P15 -to GPIO_1[20]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[20]
#set_location_assignment PIN_P16 -to GPIO_1[21]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[21]
#set_location_assignment PIN_R14 -to GPIO_1[22]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[22]
#set_location_assignment PIN_N16 -to GPIO_1[23]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[23]
#set_location_assignment PIN_N15 -to GPIO_1[24]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[24]
#set_location_assignment PIN_P14 -to GPIO_1[25]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[25]
#set_location_assignment PIN_L14 -to GPIO_1[26]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[26]
#set_location_assignment PIN_N14 -to GPIO_1[27]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[27]
#set_location_assignment PIN_M10 -to GPIO_1[28]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[28]
#set_location_assignment PIN_L13 -to GPIO_1[29]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[29]
#set_location_assignment PIN_J16 -to GPIO_1[30]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[30]
#set_location_assignment PIN_K15 -to GPIO_1[31]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[31]
#set_location_assignment PIN_J13 -to GPIO_1[32]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[32]
#set_location_assignment PIN_J14 -to GPIO_1[33]
#set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to GPIO_1[33]

#============================================================
# End of pin assignments by Terasic System Builder
#============================================================


set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top
set_global_assignment -name PARTITION_FITTER_PRESERVATION_LEVEL PLACEMENT_AND_ROUTING -section_id Top
set_global_assignment -name PARTITION_COLOR 16764057 -section_id Top
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85
set_global_assignment -name POWER_PRESET_COOLING_SOLUTION "23 MM HEAT SINK WITH 200 LFPM AIRFLOW"
set_global_assignment -name POWER_BOARD_THERMAL_MODEL "NONE (CONSERVATIVE)"
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to DRAM_DQ[*]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to DRAM_DQ[*]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to DRAM_DQM[*]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to DRAM_BA[*]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to DRAM_ADDR[*]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to DRAM_CAS_N
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to DRAM_RAS_N
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to DRAM_WE_N

set_instance_assignment -name SLEW_RATE 2 -to DRAM_DQ*

set_global_assignment -name ALLOW_ANY_RAM_SIZE_FOR_RECOGNITION ON
set_global_assignment -name SYNTH_MESSAGE_LEVEL HIGH


set_global_assignment -name VHDL_FILE ../DE10_nano_zpu_Toplevel.vhd
set_global_assignment -name QIP_FILE Clock_50to100.qip
set_global_assignment -name SDC_FILE DE10_nano_zpu_constraints.sdc
set_global_assignment -name VHDL_FILE ../cpu/zpu_core_flex.vhd
set_global_assignment -name VHDL_FILE ../cpu/zpu_pkg.vhd
set_global_assignment -name VHDL_FILE ../cpu/zpu_core_small.vhd
set_global_assignment -name VHDL_FILE ../cpu/zpu_core_medium.vhd
set_global_assignment -name VHDL_FILE ../cpu/zpu_core_evo.vhd
set_global_assignment -name VHDL_FILE ../cpu/zpu_uart_debug.vhd
set_global_assignment -name VHDL_FILE ../zpu_soc_pkg.vhd
set_global_assignment -name VHDL_FILE ../zpu_soc.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/RAM/dpram.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/uart/uart.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/intr/interrupt_controller.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/spi/spi.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/SDMMC/SDCard.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/ps2/io_ps2_com.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/timer/timer_controller.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/BRAM/BootROM.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/BRAM/DualPortBootBRAM.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/BRAM/SinglePortBootBRAM.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/BRAM/SinglePortBRAM.vhd
set_global_assignment -name VHDL_FILE ../devices/sysbus/ioctl/ioctl.vhd
#set_global_assignment -name VHDL_FILE ../devices/sysbus/TCPU/tcpu.vhd
set_global_assignment -name VHDL_FILE ../devices/WishBone/I2C/i2c_master_top.vhd
set_global_assignment -name VHDL_FILE ../devices/WishBone/I2C/i2c_master_byte_ctrl.vhd
set_global_assignment -name VHDL_FILE ../devices/WishBone/I2C/i2c_master_bit_ctrl.vhd
#set_global_assignment -name QIP_FILE ../devices/WishBone/SDRAM/sdram.qip
set_global_assignment -name VHDL_FILE ../devices/WishBone/SDRAM/sdram.vhd
set_global_assignment -name OPTIMIZATION_MODE "HIGH PERFORMANCE EFFORT"




set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id Top
