(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "Connector_Generic_Conn_02x17_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 1.27 22.86 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Connector_Generic_Conn_02x17_Odd_Even" (at 1.27 -22.86 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Connector*:*_2x??_*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Connector_Generic_Conn_02x17_Odd_Even_1_1"
      (rectangle (start -1.27 -20.193) (end 0 -20.447)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 -17.653) (end 0 -17.907)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 -15.113) (end 0 -15.367)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 -12.573) (end 0 -12.827)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 -10.033) (end 0 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 -7.493) (end 0 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 -4.953) (end 0 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 -2.413) (end 0 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 0.127) (end 0 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 2.667) (end 0 2.413)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 5.207) (end 0 4.953)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 7.747) (end 0 7.493)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 10.287) (end 0 10.033)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 12.827) (end 0 12.573)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 15.367) (end 0 15.113)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 17.907) (end 0 17.653)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 20.447) (end 0 20.193)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start -1.27 21.59) (end 3.81 -21.59)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (rectangle (start 3.81 -20.193) (end 2.54 -20.447)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -17.653) (end 2.54 -17.907)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -15.113) (end 2.54 -15.367)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -12.573) (end 2.54 -12.827)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -10.033) (end 2.54 -10.287)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -7.493) (end 2.54 -7.747)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 0.127) (end 2.54 -0.127)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 2.667) (end 2.54 2.413)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 5.207) (end 2.54 4.953)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 7.747) (end 2.54 7.493)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 10.287) (end 2.54 10.033)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 12.827) (end 2.54 12.573)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 15.367) (end 2.54 15.113)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 17.907) (end 2.54 17.653)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (rectangle (start 3.81 20.447) (end 2.54 20.193)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin passive line (at -5.08 20.32 0) (length 3.81)
        (name "Pin_1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 10.16 180) (length 3.81)
        (name "Pin_10" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 7.62 0) (length 3.81)
        (name "Pin_11" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 7.62 180) (length 3.81)
        (name "Pin_12" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 5.08 0) (length 3.81)
        (name "Pin_13" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 5.08 180) (length 3.81)
        (name "Pin_14" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 2.54 0) (length 3.81)
        (name "Pin_15" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 2.54 180) (length 3.81)
        (name "Pin_16" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 0 0) (length 3.81)
        (name "Pin_17" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 0 180) (length 3.81)
        (name "Pin_18" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -2.54 0) (length 3.81)
        (name "Pin_19" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 20.32 180) (length 3.81)
        (name "Pin_2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -2.54 180) (length 3.81)
        (name "Pin_20" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -5.08 0) (length 3.81)
        (name "Pin_21" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -5.08 180) (length 3.81)
        (name "Pin_22" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -7.62 0) (length 3.81)
        (name "Pin_23" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -7.62 180) (length 3.81)
        (name "Pin_24" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -10.16 0) (length 3.81)
        (name "Pin_25" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -10.16 180) (length 3.81)
        (name "Pin_26" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -12.7 0) (length 3.81)
        (name "Pin_27" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -12.7 180) (length 3.81)
        (name "Pin_28" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -15.24 0) (length 3.81)
        (name "Pin_29" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 17.78 0) (length 3.81)
        (name "Pin_3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -15.24 180) (length 3.81)
        (name "Pin_30" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -17.78 0) (length 3.81)
        (name "Pin_31" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -17.78 180) (length 3.81)
        (name "Pin_32" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 -20.32 0) (length 3.81)
        (name "Pin_33" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -20.32 180) (length 3.81)
        (name "Pin_34" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 17.78 180) (length 3.81)
        (name "Pin_4" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 15.24 0) (length 3.81)
        (name "Pin_5" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 15.24 180) (length 3.81)
        (name "Pin_6" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 12.7 0) (length 3.81)
        (name "Pin_7" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 12.7 180) (length 3.81)
        (name "Pin_8" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.08 10.16 0) (length 3.81)
        (name "Pin_9" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Ext_Bus_MZ800" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 31.115 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Ext_Bus_MZ800" (at 0 -31.115 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 -11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Ext_Bus_MZ800_0_0"
      (text " Top Side" (at -5.08 29.21 0)
        (effects (font (size 0.7874 0.7874)))
      )
      (text "Bottom Side" (at 3.81 29.21 0)
        (effects (font (size 0.7874 0.7874)))
      )
    )
    (symbol "Ext_Bus_MZ800_0_1"
      (rectangle (start -7.62 -29.21) (end 7.62 30.48)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "Ext_Bus_MZ800_1_1"
      (pin power_out line (at -10.16 26.67 0) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 16.51 180) (length 2.54)
        (name "D6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 13.97 0) (length 2.54)
        (name "AD15" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 13.97 180) (length 2.54)
        (name "D7" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 11.43 0) (length 2.54)
        (name "AD14" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 11.43 180) (length 2.54)
        (name "BUS0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 8.89 0) (length 2.54)
        (name "AD13" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 8.89 180) (length 2.54)
        (name "~{M1}" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 6.35 0) (length 2.54)
        (name "AD12" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 6.35 180) (length 2.54)
        (name "~{WR}" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 3.81 0) (length 2.54)
        (name "AD11" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 26.67 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 3.81 180) (length 2.54)
        (name "~{RD}" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 1.27 0) (length 2.54)
        (name "AD10" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 1.27 180) (length 2.54)
        (name "~{IORQ}" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -1.27 0) (length 2.54)
        (name "AD9" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -1.27 180) (length 2.54)
        (name "~{MREQ}" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -3.81 0) (length 2.54)
        (name "AD8" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -3.81 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -6.35 0) (length 2.54)
        (name "AD7" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -6.35 180) (length 2.54)
        (name "~{HALT}" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -8.89 0) (length 2.54)
        (name "AD6" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -10.16 24.13 0) (length 2.54)
        (name "D2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -8.89 180) (length 2.54)
        (name "IE1" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -11.43 0) (length 2.54)
        (name "AD5" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -11.43 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -13.97 0) (length 2.54)
        (name "AD4" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 -13.97 180) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -16.51 0) (length 2.54)
        (name "AD3" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -16.51 180) (length 2.54)
        (name "~{EXRESET}" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -19.05 0) (length 2.54)
        (name "AD2" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -19.05 180) (length 2.54)
        (name "~{INT}" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -21.59 0) (length 2.54)
        (name "AD1" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 24.13 180) (length 2.54)
        (name "D3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -21.59 180) (length 2.54)
        (name "~{EXWAIT}" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -10.16 -24.13 0) (length 2.54)
        (name "AD0" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -24.13 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 -26.67 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 -26.67 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -10.16 21.59 0) (length 2.54)
        (name "D1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 21.59 180) (length 2.54)
        (name "D4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -10.16 19.05 0) (length 2.54)
        (name "D0" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 19.05 180) (length 2.54)
        (name "D5" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 16.51 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "GAL22V10" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U3" (at 0 7.62 0)
      (effects (font (size 0.9906 0.9906)))
    )
    (property "Value" "GAL22V10" (at -6.35 -29.21 0)
      (effects (font (size 0.9906 0.9906)))
    )
    (property "Footprint" "Package_DIP:DIP-20_W7.62mm" (at 0 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "PAL PLD 16L8" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Programmable Logic Array, DIP-20" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP* PDIP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "GAL22V10_0_0"
      (pin power_in line (at 0 -31.75 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 19.05 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "GAL22V10_0_1"
      (rectangle (start -8.89 15.24) (end 7.62 -27.94)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "GAL22V10_1_1"
      (pin input line (at -12.7 12.7 0) (length 3.81)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 3.81)
        (name "A12" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 3.81)
        (name "A13" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 3.81)
        (name "A14" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -15.24 0) (length 3.81)
        (name "A15" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -17.78 0) (length 3.81)
        (name "~{IORQ}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -20.32 0) (length 3.81)
        (name "~{WR}" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -22.86 0) (length 3.81)
        (name "~{RD}" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -21.59 180) (length 3.81)
        (name "~{DRIVE}" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -15.24 180) (length 3.81)
        (name "~{SIDE}" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 3.81)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -8.89 180) (length 3.81)
        (name "~{RES}" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -3.81 180) (length 3.81)
        (name "~{DDEN}" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 1.27 180) (length 3.81)
        (name "~{FDC}" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 12.7 180) (length 3.81)
        (name "~{BUS}" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 3.81)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 3.81)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -25.4 0) (length 3.81)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 3.81)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 3.81)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 3.81)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 3.81)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "PAL12L6" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -8.89 16.51 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "PAL12L6" (at 1.27 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP* PDIP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PAL12L6_0_0"
      (pin power_in line (at 0 -25.4 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 19.05 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "PAL12L6_0_1"
      (rectangle (start -8.89 15.24) (end 7.62 -21.59)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "PAL12L6_1_1"
      (pin input line (at -12.7 12.7 0) (length 3.81)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 3.81)
        (name "~{WR}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -15.24 0) (length 3.81)
        (name "~{RD}" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 10.16 180) (length 3.81)
        (name "~{BUS}" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 1.27 180) (length 3.81)
        (name "~{DRIVE}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -8.89 180) (length 3.81)
        (name "~{RES}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -15.24 180) (length 3.81)
        (name "~{SIDE}" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -3.81 180) (length 3.81)
        (name "~{DDEN}" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 6.35 180) (length 3.81)
        (name "~{FDC}" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 3.81)
        (name "~{IORQ}" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 3.81)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 3.81)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 3.81)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -19.05 0) (length 3.81)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 3.81)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 3.81)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 3.81)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 3.81)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SFD700_GAL16V8_IO" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U?" (at 2.0194 18.9398 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "SFD700_GAL16V8_IO" (at 2.0194 16.4029 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP* PDIP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SFD700_GAL16V8_IO_0_0"
      (pin power_in line (at 0 -21.59 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 19.05 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SFD700_GAL16V8_IO_0_1"
      (rectangle (start -8.89 15.24) (end 7.62 -17.78)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "SFD700_GAL16V8_IO_1_1"
      (pin input line (at -12.7 12.7 0) (length 3.81)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 -12.7 180) (length 3.81)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 6.35 180) (length 3.81)
        (name "ROMA10" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 3.81)
        (name "MODE1" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 -10.16 180) (length 3.81)
        (name "ROMDIS" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 1.27 180) (length 3.81)
        (name "NA" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 3.81 180) (length 3.81)
        (name "ROMA15" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 -5.08 180) (length 3.81)
        (name "DRQ" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 3.81)
        (name "MODE0" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 8.89 180) (length 3.81)
        (name "~{ROMCS}" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 3.81)
        (name "A10" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 3.81)
        (name "A11" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 3.81)
        (name "A12" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 3.81)
        (name "A13" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 3.81)
        (name "A14" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 3.81)
        (name "A15" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 3.81)
        (name "~{MREQ}" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 3.81)
        (name "~{RD}" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SFD700_GAL16V8_MEM" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U?" (at 2.0194 18.9398 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "SFD700_GAL16V8_MEM" (at 2.0194 16.4029 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP* PDIP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SFD700_GAL16V8_MEM_0_0"
      (pin power_in line (at 0 -30.48 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 19.05 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SFD700_GAL16V8_MEM_0_1"
      (rectangle (start -8.89 15.24) (end 7.62 -30.48)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "SFD700_GAL16V8_MEM_1_1"
      (pin input line (at -12.7 12.7 0) (length 3.81)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 3.81)
        (name "A14" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 3.81)
        (name "A15" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -15.24 0) (length 3.81)
        (name "~{MREQ}" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -17.78 0) (length 3.81)
        (name "~{IORQ}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -20.32 0) (length 3.81)
        (name "~{WR}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -22.86 0) (length 3.81)
        (name "~{RD}" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -25.4 0) (length 3.81)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -5.08 180) (length 3.81)
        (name "ROMA10" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 0 180) (length 3.81)
        (name "~{DIR}" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -10.16 180) (length 3.81)
        (name "~{FDCRESET}" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -27.94 0) (length 3.81)
        (name "MODE" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 5.08 180) (length 3.81)
        (name "~{IO}" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 10.16 180) (length 3.81)
        (name "~{ROM}" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 3.81)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 3.81)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 3.81)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 3.81)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 3.81)
        (name "A10" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 3.81)
        (name "A11" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 3.81)
        (name "A12" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 3.81)
        (name "A13" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SFD700_GAL26V12_MEM" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U?" (at 2.0194 18.9398 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "SFD700_GAL26V12_MEM" (at 2.0194 16.4029 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP* PDIP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SFD700_GAL26V12_MEM_0_0"
      (pin power_in line (at 0 -31.75 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 21.59 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SFD700_GAL26V12_MEM_0_1"
      (rectangle (start -8.89 17.78) (end 7.62 -27.94)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "SFD700_GAL26V12_MEM_1_1"
      (pin input line (at -12.7 -22.86 0) (length 3.81)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 3.81)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 3.81)
        (name "~{IORQ}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -15.24 0) (length 3.81)
        (name "~{WR}" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -17.78 0) (length 3.81)
        (name "~{RD}" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 11.43 -20.32 180) (length 3.81)
        (name "ROMINH" (effects (font (size 1 1))))
        (number "14" (effects (font (size 1 1))))
      )
      (pin output line (at 11.43 -15.24 180) (length 3.81)
        (name "DISROMSET" (effects (font (size 1 1))))
        (number "15" (effects (font (size 1 1))))
      )
      (pin output line (at 11.43 -17.78 180) (length 3.81)
        (name "DISROMCLR" (effects (font (size 1 1))))
        (number "16" (effects (font (size 1 1))))
      )
      (pin output line (at -12.7 -25.4 0) (length 3.81)
        (name "INTCLK" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -10.16 180) (length 3.81)
        (name "INHROMSET" (effects (font (size 1 1))))
        (number "18" (effects (font (size 1 1))))
      )
      (pin output line (at 11.43 -6.35 180) (length 3.81)
        (name "INTEN" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 12.7 0) (length 3.81)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -3.81 180) (length 3.81)
        (name "~{IOBUSDIR}" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -12.7 180) (length 3.81)
        (name "INHROMCLR" (effects (font (size 1 1))))
        (number "22" (effects (font (size 1 1))))
      )
      (pin output line (at 11.43 -1.27 180) (length 3.81)
        (name "~{SIDE}" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 1.27 180) (length 3.81)
        (name "~{FDCRESET}" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 3.81 180) (length 3.81)
        (name "~{DDEN}" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 6.35 180) (length 3.81)
        (name "~{DRIVE}" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 8.89 180) (length 3.81)
        (name "~{FDC}" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -20.32 0) (length 3.81)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 3.81)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 3.81)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 3.81)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 3.81)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 3.81)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 3.81)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SFD700_PAL12L6" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -8.89 16.51 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "SFD700_PAL12L6" (at 1.27 17.78 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP* PDIP*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SFD700_PAL12L6_0_0"
      (pin power_in line (at 0 -25.4 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 19.05 270) (length 3.81)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "SFD700_PAL12L6_0_1"
      (rectangle (start -8.89 15.24) (end 7.62 -21.59)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "SFD700_PAL12L6_1_1"
      (pin input line (at -12.7 12.7 0) (length 3.81)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -12.7 0) (length 3.81)
        (name "~{WR}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -15.24 0) (length 3.81)
        (name "~{RD}" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 10.16 180) (length 3.81)
        (name "~{BUS}" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 1.27 180) (length 3.81)
        (name "~{DRIVE}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -8.89 180) (length 3.81)
        (name "~{RES}" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -15.24 180) (length 3.81)
        (name "~{SIDE}" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -3.81 180) (length 3.81)
        (name "~{DDEN}" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 6.35 180) (length 3.81)
        (name "~{FDC}" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 3.81)
        (name "~{IORQ}" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 3.81)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 3.81)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 3.81)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -19.05 0) (length 3.81)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.54 0) (length 3.81)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 0 0) (length 3.81)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 3.81)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 3.81)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "W27C512" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 26.67 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "W27C512" (at -11.43 -17.78 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DIP:DIP-28_W15.24mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -3.81 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "OTP EPROM 512KiBit" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "OTP EPROM 512 KiBit" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W15.24mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "W27C512_1_1"
      (rectangle (start -7.62 24.13) (end 7.62 -16.51)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -10.16 -15.24 0) (length 2.54)
        (name "A15" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 22.86 0) (length 2.54)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 22.86 180) (length 2.54)
        (name "D0" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 20.32 180) (length 2.54)
        (name "D1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 17.78 180) (length 2.54)
        (name "D2" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -19.05 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 15.24 180) (length 2.54)
        (name "D3" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 12.7 180) (length 2.54)
        (name "D4" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 10.16 180) (length 2.54)
        (name "D5" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 7.62 180) (length 2.54)
        (name "D6" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 5.08 180) (length 2.54)
        (name "D7" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -7.62 0) (length 2.54)
        (name "A12" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -12.7 180) (length 2.54)
        (name "~{CE}" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "A10" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 10.16 -15.24 180) (length 2.54)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "A11" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "A9" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "A8" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -10.16 0) (length 2.54)
        (name "A13" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -12.7 0) (length 2.54)
        (name "A14" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 26.67 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 10.16 0) (length 2.54)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 12.7 0) (length 2.54)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 17.78 0) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 20.32 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "WD1773" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U13" (at 0 5.08 0)
      (effects (font (size 0.9906 0.9906)))
    )
    (property "Value" "WD1773" (at -7.62 -26.67 0)
      (effects (font (size 0.9906 0.9906)))
    )
    (property "Footprint" "Package_DIP:DIP-28_W15.24mm" (at 19.05 -29.21 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://amaus.net/static/S100/western%20digital/datasheet/Western%20Digital%20FD1771%20Specification%20197710.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W15.24mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "WD1773_0_1"
      (rectangle (start -10.16 21.59) (end 10.16 -25.4)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "WD1773_1_1"
      (pin input line (at -12.7 -13.97 0) (length 2.54)
        (name "~{CS}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 1.27 0) (length 2.54)
        (name "DI5" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 -1.27 0) (length 2.54)
        (name "DI6" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 -3.81 0) (length 2.54)
        (name "DI7" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 17.78 0) (length 2.54)
        (name "~{MR}" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -27.94 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 24.13 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 10.16 180) (length 2.54)
        (name "STEP" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 12.7 180) (length 2.54)
        (name "DIRC" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input clock (at 12.7 17.78 180) (length 2.54)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -6.35 180) (length 2.54)
        (name "~{RD}" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -16.51 0) (length 2.54)
        (name "R/~{W}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -13.97 180) (length 2.54)
        (name "RDY/ENP" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 2.54 180) (length 2.54)
        (name "WG" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 5.08 180) (length 2.54)
        (name "WD" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -3.81 180) (length 2.54)
        (name "~{TR00}" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -8.89 180) (length 2.54)
        (name "~{IP}" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -11.43 180) (length 2.54)
        (name "~{WPRT}" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -22.86 180) (length 2.54)
        (name "~{DDEN}" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 -22.86 0) (length 2.54)
        (name "DRQ" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -12.7 -20.32 0) (length 2.54)
        (name "INTRQ" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.62 0) (length 2.54)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -10.16 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 13.97 0) (length 2.54)
        (name "DI0" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 11.43 0) (length 2.54)
        (name "DI1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 8.89 0) (length 2.54)
        (name "DI2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 6.35 0) (length 2.54)
        (name "DI3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at -12.7 3.81 0) (length 2.54)
        (name "DI4" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
